(footprint "easyeda2kicad:CONN-SMD_B2B-PH-SM4-TBT-LF-SN"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -5.12 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "f1c6fd17-f458-4b60-8df5-00e09e398f8c")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "CONN-SMD_B2B-PH-SM4-TBT-LF-SN"
        (at 0 5.12 0)
        (layer "F.Fab")
        (hide no)
        (uuid "53bcdd7e-3c13-4525-a7c4-44fa41b63003")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (attr smd)
    (fp_line
        (start -4 -3.63)
        (end 4 -3.63)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "30641db5-9964-4671-855a-0d94cf1be66a")
    )
    (fp_line
        (start -4 1.37)
        (end -1.73 1.37)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "c0b22978-fd80-4fd5-bdc3-7a62f9c71684")
    )
    (fp_line
        (start -0.27 1.37)
        (end 0.27 1.37)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "822fe15c-15a9-488c-bbf3-0e384e836f8b")
    )
    (fp_line
        (start 1.73 1.37)
        (end 4 1.37)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "bbb530c7-462d-42c8-ad26-cb6ff786b863")
    )
    (fp_line
        (start 4 1.37)
        (end 4 0.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "fcfe6d36-2516-4eb8-9caf-c55c43212090")
    )
    (fp_line
        (start 4 -2.86)
        (end 4 -3.63)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "d0b4f0db-64a2-4893-be7b-e0417c3c0dd3")
    )
    (fp_line
        (start -4 -3.63)
        (end -4 -2.86)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "72e9119c-8ca6-434b-96d2-3d5731f876ba")
    )
    (fp_line
        (start -4 0.6)
        (end -4 1.37)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "94d03034-fbdc-47a4-a7bc-aaf06a4c889f")
    )
    (fp_circle
        (center -3.97 3.38)
        (end -3.94 3.38)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "b19e2870-65e6-443e-8c84-899299d4b156")
    )
    (fp_circle
        (center -0.95 3.07)
        (end -0.82 3.07)
        (stroke
            (width 0.25)
            (type solid)
        )
        (fill no)
        (layer "Cmts.User")
        (uuid "ce18044f-e079-4527-a32c-9f78b1eed09a")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "ae17cc2e-b204-4a94-be5f-e57ca9558c51")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -5.12 0)
        (layer "F.SilkS")
        (uuid "f1c6fd17-f458-4b60-8df5-00e09e398f8c")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "1" smd rect
        (at -1 1.12 0)
        (size 1 5.5)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "c16bb4aa-8ef7-432f-a49d-c6c32f5391e5")
    )
    (pad "2" smd rect
        (at 1 1.12 0)
        (size 1 5.5)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "ad5511c4-fa78-461e-964e-9de6eea69c99")
    )
    (pad "3" smd rect
        (at 3.5 -1.12 0)
        (size 2 3)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "7474c68e-8312-415f-bf65-71ed1771361d")
    )
    (pad "4" smd rect
        (at -3.5 -1.12 0)
        (size 2 3)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "648ef6f5-05e3-43fd-bd06-98078cc639fc")
    )
    (model "${KIPRJMOD}/../../build/cache/parts/easyeda/C265003/CONN-SMD_B2B-PH-SM4-TBT-LF-SN.step"
        (offset
            (xyz 0 0 0)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 0)
        )
    )
)