(footprint "PANASONIC_EEEFK1A471AP:CAP-SMD_BD8.0-L8.3-W8.3-LS9.9-FD"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -4 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "623ea059-aff4-4353-aaf8-8b5f597349bf")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "CAP-SMD_BD8.0-L8.3-W8.3-LS9.9-FD"
        (at 0 4 0)
        (layer "F.Fab")
        (hide no)
        (uuid "edd08b58-caf8-4cc1-afc3-307a4b958dbe")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "checksum" "3a30aba91912392ddab4b95cf4c5624802b3c2048a8d62eb75165e8d2cddd84a"
        (at 0 0 0)
        (layer "User.9")
        (hide no)
        (uuid "8c3ea71c-3b17-46b5-8887-cde37fc138d0")
        (effects
            (font
                (size 0.125 0.125)
                (thickness 0.01875)
            )
            (hide yes)
        )
    )
    (attr smd)
    (fp_line
        (start 4.2 0.78)
        (end 4.2 4.23)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "7d872c1b-d9e7-49dc-92ab-9bcae2358fff")
    )
    (fp_line
        (start 4.2 4.23)
        (end -2.46 4.23)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "ee682e10-4e8e-4ece-ba53-ae3d8778abaa")
    )
    (fp_line
        (start -2.46 4.23)
        (end -4.2 2.49)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "e6798260-0ce2-41f1-b2f3-9e99838a29a4")
    )
    (fp_line
        (start -4.2 2.49)
        (end -4.2 0.78)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "2c977140-e2a0-480f-b30a-b9d26b6986aa")
    )
    (fp_line
        (start 4.2 -0.78)
        (end 4.2 -4.23)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "7b182ed0-6e93-48b4-8e41-e144aa20b298")
    )
    (fp_line
        (start 4.2 -4.23)
        (end -2.46 -4.23)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "ab041e32-8109-4b1c-b56b-32d3e8d87c2e")
    )
    (fp_line
        (start -2.46 -4.23)
        (end -4.2 -2.49)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "339f79a3-2602-4119-804e-f418a9ad5670")
    )
    (fp_line
        (start -4.2 -2.49)
        (end -4.2 -0.78)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "94991dbb-c964-4563-99e5-af6404401655")
    )
    (fp_circle
        (center -4.95 4.15)
        (end -4.92 4.15)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "93fb89ed-b399-4512-b84a-c132e4b74c7a")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "fab31861-4a29-436f-acfb-d057f1eedb26")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -4 0)
        (layer "F.SilkS")
        (uuid "623ea059-aff4-4353-aaf8-8b5f597349bf")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "2" smd rect
        (at 3.6 0 0)
        (size 4.3 1.26)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "91f18ca7-ce55-4fd0-b3cc-a3af30352a21")
    )
    (pad "1" smd rect
        (at -3.6 0 0)
        (size 4.3 1.26)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "3aa34514-5a54-4e7d-8ebd-6078bca838b8")
    )
    (model "${KIPRJMOD}/../../parts/PANASONIC_EEEFK1A471AP/CAP-SMD_BD8.0-L8.3-W8.3-LS9.9-FD.step"
        (offset
            (xyz 0 0 0)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 180)
        )
    )
)