(kicad_pcb
    (version 20241229)
    (generator "atopile")
    (generator_version "0.12.4")
    (general
        (thickness 1.6)
        (legacy_teardrops no)
    )
    (paper "A4")
    (layers
        (0 "F.Cu" signal)
        (31 "B.Cu" signal)
        (32 "B.Adhes" user "B.Adhesive")
        (33 "F.Adhes" user "F.Adhesive")
        (34 "B.Paste" user)
        (35 "F.Paste" user)
        (36 "B.SilkS" user "B.Silkscreen")
        (37 "F.SilkS" user "F.Silkscreen")
        (38 "B.Mask" user)
        (39 "F.Mask" user)
        (40 "Dwgs.User" user "User.Drawings")
        (41 "Cmts.User" user "User.Comments")
        (42 "Eco1.User" user "User.Eco1")
        (43 "Eco2.User" user "User.Eco2")
        (44 "Edge.Cuts" user)
        (45 "Margin" user)
        (46 "B.CrtYd" user "B.Courtyard")
        (47 "F.CrtYd" user "F.Courtyard")
        (48 "B.Fab" user)
        (49 "F.Fab" user)
        (50 "User.1" user)
        (51 "User.2" user)
        (52 "User.3" user)
        (53 "User.4" user)
        (54 "User.5" user)
        (55 "User.6" user)
        (56 "User.7" user)
        (57 "User.8" user)
        (58 "User.9" user)
    )
    (setup
        (pad_to_mask_clearance 0)
        (allow_soldermask_bridges_in_footprints no)
        (pcbplotparams
            (layerselection 0x00010fc_ffffffff)
            (plot_on_all_layers_selection 0x0000000_00000000)
            (disableapertmacros no)
            (usegerberextensions no)
            (usegerberattributes yes)
            (usegerberadvancedattributes yes)
            (creategerberjobfile yes)
            (dashed_line_dash_ratio 12)
            (dashed_line_gap_ratio 3)
            (svgprecision 4)
            (plotframeref no)
            (mode 1)
            (useauxorigin no)
            (hpglpennumber 1)
            (hpglpenspeed 20)
            (hpglpendiameter 15)
            (pdf_front_fp_property_popups yes)
            (pdf_back_fp_property_popups yes)
            (dxfpolygonmode yes)
            (dxfimperialunits yes)
            (dxfusepcbnewfont yes)
            (psnegative no)
            (psa4output no)
            (plot_black_and_white yes)
            (plotinvisibletext no)
            (sketchpadsonfab no)
            (plotreference yes)
            (plotvalue yes)
            (plotpadnumbers no)
            (hidednponfab no)
            (sketchdnponfab yes)
            (crossoutdnponfab yes)
            (plotfptext yes)
            (subtractmaskfromsilk no)
            (outputformat 1)
            (mirror no)
            (drillshape 1)
            (scaleselection 1)
            (outputdirectory "")
        )
    )
    (net 0 "")
    (net 1 "footprint-net-0")
    (net 2 "footprint-net-1")
    (footprint "UNI_ROYAL_0402WGF1001TCE:R0402"
        (layer "F.Cu")
        (uuid "3786f3ed-0717-40b7-878c-fb2e4642524b")
        (at 0 0 0)
        (property "Reference" "R1"
            (at 0 -4 0)
            (layer "F.SilkS")
            (hide no)
            (uuid "345f7ad1-a349-47f8-ba4e-04bbff791b4c")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" "1kΩ ±1% 62.5mW"
            (at 0 4 0)
            (layer "F.Fab")
            (hide no)
            (uuid "5bb0bb1f-f910-443d-8b36-165244157542")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "3a0ec2dc7c35c97972db9e2a5c9a26a9a2b74cc9defe80a40041b96130696053"
            (at 0 0 0)
            (layer "User.9")
            (hide no)
            (uuid "228f17e1-2a4f-463e-8e0f-87da090f4dac")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
                (hide yes)
            )
        )
        (property "__atopile_lib_fp_hash__" "7c45da14-3bc9-9ff3-ac7d-f87868332dd6"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "c36e4ece-d26c-49bd-bd6f-96f74642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C11702"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "09a3d748-723f-497c-b808-a6e94642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "UNI-ROYAL(Uniroyal Elec)"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "1925f3ba-5569-4353-83e2-ed744642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "0402WGF1001TCE"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "bdaf9cd6-1532-4adc-95ad-9ea14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "PARAM_max_power" "{\"type\": \"Quantity_Set_Discrete\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 0.0625, \"max\": 0.0625}}]}}, \"unit\": \"watt\"}}"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "f44a19a0-9a0e-4b1c-82a7-1d954642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "PARAM_max_voltage" "{\"type\": \"Quantity_Set_Discrete\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 50.0, \"max\": 50.0}}]}}, \"unit\": \"volt\"}}"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "71ce1f69-2f47-4075-8b6b-28514642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "PARAM_resistance" "{\"type\": \"Quantity_Interval_Disjoint\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 990.0000002235174, \"max\": 1009.9999997764826}}]}}, \"unit\": \"ohm\"}}"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "8787dca7-1715-43a7-ac17-397a4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010216_UNI-ROYAL-Uniroyal-Elec-0402WGF1001TCE_C11702.pdf"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "fca7427a-a81f-4bc7-8763-b7774642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "r1"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "61c60446-608d-45d8-9ad5-1ce14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -0.23 0.5)
            (end -0.94 0.5)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "21b359e6-90b8-4fb8-853e-add0723cddbe")
        )
        (fp_line
            (start -0.94 0.5)
            (end -0.94 -0.5)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "4d115620-9f34-4a4c-acfc-573024bf8391")
        )
        (fp_line
            (start -0.94 -0.5)
            (end -0.23 -0.5)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "3b973153-847e-422b-a3c7-8b1b9197d5f9")
        )
        (fp_line
            (start 0.23 0.5)
            (end 0.94 0.5)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "a50adf3b-7d8d-44e9-ae20-37d2d5ec6c3f")
        )
        (fp_line
            (start 0.94 0.5)
            (end 0.94 -0.5)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "97e20f73-6781-4bb7-9ebc-56c6b6e9b7ef")
        )
        (fp_line
            (start 0.94 -0.5)
            (end 0.23 -0.5)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "c39c83d4-6820-4c61-948f-b26adff78450")
        )
        (fp_circle
            (center -0.5 0.25)
            (end -0.47 0.25)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "36beed3a-b303-47b4-8a79-76d673e00205")
        )
        (fp_text user "%R"
            (at 0 0 0)
            (layer "F.Fab")
            (uuid "161b6753-2c5b-4310-aaec-4b75c042bc2f")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 -4 0)
            (layer "F.SilkS")
            (uuid "345f7ad1-a349-47f8-ba4e-04bbff791b4c")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "2" smd rect
            (at 0.43 0 0)
            (size 0.57 0.54)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 2 "footprint-net-1")
            (uuid "89f48650-ba2e-4c63-891a-4008dc400372")
        )
        (pad "1" smd rect
            (at -0.43 0 0)
            (size 0.57 0.54)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 1 "footprint-net-0")
            (uuid "1d8e8538-3920-49c9-b964-a4be4e5a7d17")
        )
        (model "${KIPRJMOD}/../../parts/UNI_ROYAL_0402WGF1001TCE/R0402_L1.0-W0.5-H0.4.step"
            (offset
                (xyz 0 0 0)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 0)
            )
        )
    )
)