(footprint "easyeda2kicad:AUDIO-SMD_HANELECTRICITY_PJ-320D"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -8.3 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "c369c749-deb9-447c-a14d-ffff7cb82a53")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "AUDIO-SMD_HANELECTRICITY_PJ-320D"
        (at 0 8.3 0)
        (layer "F.Fab")
        (hide no)
        (uuid "f85375fe-fa1b-45b9-9434-3ca72a7d910f")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (attr smd)
    (fp_line
        (start 3.13 3.63)
        (end 3.13 4.8)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "e6a91fa8-3fea-4d84-9cc2-02846e7845c6")
    )
    (fp_line
        (start 3.13 4.8)
        (end -1.77 4.8)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "e73963f1-ab79-4185-a52e-a038c08309f1")
    )
    (fp_line
        (start -2.5 -9.5)
        (end 2.5 -9.5)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "0e51fa23-41b9-48a1-8aef-ca426d1dc955")
    )
    (fp_line
        (start -3.12 -7.5)
        (end -3.12 2.94)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "6f658083-cf6b-4a42-9a3f-11e6d3e25e1f")
    )
    (fp_line
        (start 3.13 -7.49)
        (end 3.13 -5.23)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "87072722-f0ae-4829-bef9-8ffae0025ed5")
    )
    (fp_line
        (start 3.13 -7.5)
        (end -3.12 -7.5)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "4d32968c-0f68-4cd7-919c-f363097defe0")
    )
    (fp_line
        (start -2.5 -9.5)
        (end -2.5 -7.5)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "11b6d962-5cfb-4b39-b6d8-414fc8f22088")
    )
    (fp_line
        (start 2.5 -7.5)
        (end 2.5 -9.5)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "8d1c1c18-4df1-4295-b77c-746c6f880f9f")
    )
    (fp_line
        (start 3.13 -0.37)
        (end 3.13 1.77)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "a2bf6611-c16d-4513-987c-c24c9bb0a1be")
    )
    (fp_line
        (start 3.13 -3.37)
        (end 3.13 -2.23)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "3f93233e-abe1-4ddd-8c8e-0ce4b53068ec")
    )
    (fp_circle
        (center -4 4.8)
        (end -3.97 4.8)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "54a9e815-6675-4f38-9c49-0bef370e0fc2")
    )
    (fp_circle
        (center 0 -5.8)
        (end 0.2 -5.8)
        (stroke
            (width 0.4)
            (type solid)
        )
        (fill no)
        (layer "Cmts.User")
        (uuid "62324c56-a399-4082-ba8b-7ac73739c650")
    )
    (fp_circle
        (center 0 1.2)
        (end 0.2 1.2)
        (stroke
            (width 0.4)
            (type solid)
        )
        (fill no)
        (layer "Cmts.User")
        (uuid "75038695-8698-4b40-ab4b-46164f7e788d")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "e7c68e98-fd65-48e8-b01f-3b3f303adb6b")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -8.3 0)
        (layer "F.SilkS")
        (uuid "c369c749-deb9-447c-a14d-ffff7cb82a53")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "2" smd rect
        (at 3.5 -4.3 0)
        (size 3 1.4)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "44f55399-ebd8-4457-ab68-e0d0137f646b")
    )
    (pad "3" smd rect
        (at 3.5 -1.3 0)
        (size 3 1.4)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "087422cf-bb6d-4015-afa1-3631eef1f332")
    )
    (pad "4" smd rect
        (at 3.5 2.7 0)
        (size 3 1.4)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "40a78dc6-3693-46fb-9f4f-af1afa735eec")
    )
    (pad "1" smd rect
        (at -3.5 4.3 0)
        (size 3 1.4)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "54caf76f-591a-4801-80f4-0026d46819b4")
    )
    (pad "" thru_hole circle
        (at 0 -5.8 0)
        (size 1.4 1.4)
        (drill 1.4)
        (layers "*.Cu" "*.Mask")
        (uuid "9d5b0166-9a8f-4eec-b7fc-df0ab60ef3a3")
    )
    (pad "" thru_hole circle
        (at 0 1.2 0)
        (size 1.4 1.4)
        (drill 1.4)
        (layers "*.Cu" "*.Mask")
        (uuid "d59a4a86-e61c-4db5-acc0-133b6d747031")
    )
    (model "${KIPRJMOD}/../../build/cache/parts/easyeda/C22459515/AUDIO-SMD_HANELECTRICITY_PJ-320D.step"
        (offset
            (xyz 0 0 1)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 180)
        )
    )
)