[00:52:32] INFO     Loading KiCad PCB file: /home/martin/proj/DFPlayerMB/layout/default/default.kicad_pcb                                                                                                                                                                                                                                                                                                                                                                                                           
           INFO     Decode Error                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    
                    Failed to decode file /home/martin/proj/DFPlayerMB/layout/default/default.kicad_pcb                                                                                                                                                                                                                                                                                                                                                                                                             
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    
                    Failed to create C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint:                                                                                                                                                                                                                                                                                                                                                                                                                                  
                    C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.__init__() missing 1 required keyword-only argument: 'attr' with                                                                                                                                                                                                                                                                                                                                                                                   
                    - **unknown:** None                                                                                                                                                                                                                                                                                                                                                                                                                                                                             
                    - **layer:** F.Cu                                                                                                                                                                                                                                                                                                                                                                                                                                                                               
                    - **propertys:** {'Reference': C_footprint.C_property(name='Reference', value='H1', at=C_xyr(x=0.0, y=-5.5, r=0.0), layer=C_text_layer(layer='F.SilkS', knockout=None), hide=False, uuid='e1fdcb25-bbb7-480b-a3eb-ca2182d4a17c', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=1.0, h=1.0), thickness=0.15, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), 'Value': C_footprint.C_property(name='Value', value='',            
                    at=C_xyr(x=0.0, y=5.5, r=0.0), layer=C_text_layer(layer='F.Fab', knockout=None), hide=False, uuid='e6735211-f1b3-4a8d-a8a6-ddd8d9cce98f', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=1.0, h=1.0), thickness=0.15, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), 'Datasheet': C_footprint.C_property(name='Datasheet', value='', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='F.Fab', knockout=None),          
                    hide=True, uuid='b609117e-058c-4c2e-a923-ab17bf02f4dd', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=1.27, h=1.27), thickness=0.15, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), 'Description': C_footprint.C_property(name='Description', value='', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='F.Fab', knockout=None), hide=True, uuid='34c3213a-e7b2-4932-945d-3a84597506b1',                              
                    effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=1.27, h=1.27), thickness=0.15, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), 'checksum': C_footprint.C_property(name='checksum', value='e1ae12f555519af8c11439d0a2175ddbbdd080e821244f82aff68eb0bebf1f55', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='User.9', knockout=None), hide=True, uuid='c57eb9dc-59b1-4c0a-a46a-ca4b82054a05',                           
                    effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=0.125, h=0.125), thickness=0.01875, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), '__atopile_lib_fp_hash__': C_footprint.C_property(name='__atopile_lib_fp_hash__', value='0eae38e2-f249-5e39-dd2b-1da477ebfd1d', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='User.9', knockout=None), hide=True, uuid='6e61aa35-c501-45e5-8d08-1b7e4642524b',                    
                    effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=0.125, h=0.125), thickness=0.01875, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), 'LCSC': C_footprint.C_property(name='LCSC', value='C48641756', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='User.9', knockout=None), hide=True, uuid='47dfa67e-ed26-42a1-9f05-26774642524b', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None,                
                    size=C_wh(w=0.125, h=0.125), thickness=0.01875, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])), 'Manufacturer': C_footprint.C_property(name='Manufacturer', value='hanxia', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='User.9', knockout=None), hide=True, uuid='00f59694-8ebe-4b4f-a19f-c83b4642524b', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=0.125, h=0.125), thickness=0.01875, bold=None, italic=None,
                    unresolved_font_name=None), hide=None, justifys=[])), 'Partnumber': C_footprint.C_property(name='Partnumber', value='HX PM2.54-1x8P TP H8.5-ZQ', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='User.9', knockout=None), hide=True, uuid='89e98553-d3d0-479b-8ff0-64114642524b', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=0.125, h=0.125), thickness=0.01875, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[])),   
                    'atopile_address': C_footprint.C_property(name='atopile_address', value='df_header_left', at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='User.9', knockout=None), hide=True, uuid='c0bd2da2-48d8-49e5-a9c5-66084642524b', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=0.125, h=0.125), thickness=0.01875, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[]))}                                                          
                    - **fp_lines:** [C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='a3d6dfd4-6734-4927-a957-05e3dc6140ce', start=C_xy(x=-10.16, y=-1.27), end=C_xy(x=-7.22, y=-1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='1bd1ae5a-0142-45fa-a407-9206686723ba', start=C_xy(x=-10.16,   
                    y=1.27), end=C_xy(x=-10.16, y=-1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='0614385d-9bf9-4ef3-82b6-a83d514d87c4', start=C_xy(x=-9.75, y=1.27), end=C_xy(x=-10.16, y=1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='7a1d7a0e-7ce5-46b1-aeb4-0c8fdc0b5e5d',    
                    start=C_xy(x=-5.49, y=-1.27), end=C_xy(x=-2.13, y=-1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='9664ed60-714e-4f63-960a-b936fc4647d3', start=C_xy(x=-4.67, y=1.27), end=C_xy(x=-8.02, y=1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None,                              
                    uuid='219acf0c-bff7-4e14-9c0d-4aa72300865e', start=C_xy(x=-0.4, y=-1.27), end=C_xy(x=2.95, y=-1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='6a3c726a-a4fb-4db1-9faf-10daa681229f', start=C_xy(x=0.4, y=1.27), end=C_xy(x=-2.95, y=1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None,  
                    locked=None, uuid='88260e44-03bb-472a-b0b7-bfc980f8a560', start=C_xy(x=4.67, y=-1.27), end=C_xy(x=8.02, y=-1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='92270ee3-3b03-4d15-89cc-25d42e1a68f2', start=C_xy(x=5.49, y=1.27), end=C_xy(x=2.13, y=1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>),
                    fill=None, locked=None, uuid='e2696bdc-e1af-410c-bf01-70efd20c9991', start=C_xy(x=7.22, y=1.27), end=C_xy(x=10.15, y=1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='9fe7b994-fabf-4967-ba95-ba1ef22ac473', start=C_xy(x=10.15, y=-1.27), end=C_xy(x=9.75, y=-1.27)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25,                  
                    type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='bd068a07-dcf1-4279-82e5-2be285c6b171', start=C_xy(x=10.15, y=-1.27), end=C_xy(x=10.15, y=-0.51)), C_line(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.25, type=<E_type.solid: 'solid'>), fill=None, locked=None, uuid='3041c736-cad2-4538-a405-217b0583e46d', start=C_xy(x=10.15, y=-0.51), end=C_xy(x=10.15, y=1.27))]                                                                          
                    - **fp_circles:** [C_circle(layer='F.SilkS', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.3, type=<E_type.solid: 'solid'>), fill=<E_fill.no: 'no'>, locked=None, uuid='57cc6a1d-bd3d-43bb-bd86-97116c66cfd0', center=C_xy(x=-10.16, y=2.54), end=C_xy(x=-10.01, y=2.54)), C_circle(layer='F.Fab', layers=None, solder_mask_margin=None, stroke=C_stroke(width=0.06, type=<E_type.solid: 'solid'>), fill=<E_fill.no: 'no'>, locked=None,                                        
                    uuid='9f95cfa0-d1bd-4315-9a64-26c9896bacbd', center=C_xy(x=-10.16, y=2.4), end=C_xy(x=-10.13, y=2.4))]                                                                                                                                                                                                                                                                                                                                                                                          
                    - **fp_texts:** [C_fp_text(type=<E_type.user: 'user'>, text='${REFERENCE}', at=C_xyr(x=0.0, y=-5.5, r=0.0), layer=C_text_layer(layer='F.SilkS', knockout=None), hide=None, uuid='22e6a931-c2c4-412d-a27b-dfb98dca363a', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=1.0, h=1.0), thickness=0.15, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[]), unlocked=False), C_fp_text(type=<E_type.user: 'user'>, text='${REFERENCE}',  
                    at=C_xyr(x=0.0, y=0.0, r=0.0), layer=C_text_layer(layer='F.Fab', knockout=None), hide=None, uuid='aa94f2c5-ea48-45ac-abb9-17c29da40240', effects=C_fp_text.C_fp_text_effects(font=C_effects.C_font(face=None, size=C_wh(w=1.0, h=1.0), thickness=0.15, bold=None, italic=None, unresolved_font_name=None), hide=None, justifys=[]), unlocked=False)]                                                                                                                                            
                    - **pads:** [C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='1', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=-8.89, y=1.5, r=180.0), size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None,           
                    thermal_gap=None, roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=16, name='v_dfplayer'), options=None, padstack=None, remove_unused_layers=None, keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='0b4a9f64-89fe-4b66-af32-c2df7be08c09', unknown=None), C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='2', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=-6.35, y=-1.5, r=180.0),       
                    size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None, roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=22, name='df_header_left-_2-0'), options=None, padstack=None,            
                    remove_unused_layers=None, keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='5094a899-3132-4fb1-92b2-b23f8a7f1ac2', unknown=None), C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='3', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=-3.81, y=1.5, r=180.0), size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None,         
                    solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None, roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=17, name='df_header_left-_3'), options=None, padstack=None, remove_unused_layers=None, keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='418d2820-79dd-4774-89ec-5e1cc2077416', unknown=None),                       
                    C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='4', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=-1.27, y=-1.5, r=180.0), size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None,     
                    roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=19, name='df_header_left-_1-0'), options=None, padstack=None, remove_unused_layers=None, keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='ce158f8c-ef79-4474-bb57-93b0ae7cd8e2', unknown=None), C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='5', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=1.27, y=1.5, r=180.0), size=C_wh(w=1.02,
                    h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None, roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=15, name='df_header_left-_2-1'), options=None, padstack=None, remove_unused_layers=None,   
                    keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='5d145eb8-cce2-4595-a38a-b1acf7fe4c95', unknown=None), C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='6', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=3.81, y=-1.5, r=180.0), size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None,    
                    clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None, roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=12, name='df_header_left-_1-1'), options=None, padstack=None, remove_unused_layers=None, keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='37c4b44f-eb20-43a8-ac8a-94d7ec55b7cd', unknown=None),                                                     
                    C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='7', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=6.35, y=1.5, r=180.0), size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None,       
                    roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=10, name='df_header_left-_2-2'), options=None, padstack=None, remove_unused_layers=None, keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='46c85612-6230-4434-b26f-8fbad3d5b776', unknown=None), C_kicad_pcb_file.C_kicad_pcb.C_pcb_footprint.C_pad_no_net(name='8', type=<E_type.smd: 'smd'>, shape=<E_shape.rect: 'rect'>, at=C_xyr(x=8.89, y=-1.5, r=180.0),                 
                    size=C_wh(w=1.02, h=3.0), rect_delta=None, drill=None, layers=['F.Cu', 'F.Mask', 'F.Paste'], die_length=None, solder_mask_margin=None, solder_paste_margin=None, solder_paste_margin_ratio=None, clearance=None, teardrops=None, zone_connect=None, thermal_bridge_width=None, thermal_bridge_angle=None, thermal_gap=None, roundrect_rratio=None, chamfer_ratio=None, chamfer=None, properties=None, net=C_net(number=11, name='gnd'), options=None, padstack=None, remove_unused_layers=None, 
                    keep_end_layers=None, tenting=None, zone_layer_connections=None, uuid='30e38b82-4508-4f5d-bdee-a1985b0077eb', unknown=None)]                                                                                                                                                                                                                                                                                                                                                                    
                    - **embedded_fonts:** no                                                                                                                                                                                                                                                                                                                                                                                                                                                                        
                    - **uuid:** bfe8ac0a-d3cd-4e7c-9a0f-6ff64642524b                                                                                                                                                                                                                                                                                                                                                                                                                                                
                    - **at:** C_xyr(x=153.11, y=102.5, r=0)                                                                                                                                                                                                                                                                                                                                                                                                                                                         
                    - **name:** hanxia_HX_PM2_54_1x8P_TP_H8_5_ZQ:HDR-SMD_8P-P2.54-V-F-LS4.7                                                                                                                                                                                                                                                                                                                                                                                                                         
           INFO     Loading KiCad PCB file (header): /home/martin/proj/DFPlayerMB/layout/default/default.kicad_pcb                                                                                                                                                                                                                                                                                                                                                                                                  
