## Exporting gcode files from KiCad

Adapt milling and drilling parameters in `millproject`:
```bash
nano millproject
```

Run the export by providing the .kicad_pcb file as a first argument:

```bash
chmod +x export.sh
./export.sh Step_Down_Carrier_Board.kicad_pcb
```
The script will generate gerber files in the `output` directory and then convert them into `ngc` format in the `gcode` directory.

Load the `ngc` file to `gSender` program for the fabrication.

