(export
    (version "E")
    (components
        (comp
            (ref "C1")
            (value "Elec_Cap_6_3x5_4")
            (footprint "PANASONIC_EEEFK1A471AP:CAP-SMD_BD8.0-L8.3-W8.3-LS9.9-FD")
            (property
                (name "LCSC")
                (value "C178529")
            )
            (property
                (name "Manufacturer")
                (value "PANASONIC")
            )
            (property
                (name "Partnumber")
                (value "EEEFK1A471AP")
            )
            (property
                (name "atopile_address")
                (value "power_filter_cap")
            )
            (tstamps "1")
            (fields)
        )
        (comp
            (ref "CN1")
            (value "JST_PH_Vertical_4Pin")
            (footprint "JST_Sales_America_B4B_PH_SM4_TB_LF__SN:CONN-SMD_B4B-PH-SM4-TB-LF-SN")
            (property
                (name "LCSC")
                (value "C160354")
            )
            (property
                (name "Manufacturer")
                (value "JST Sales America")
            )
            (property
                (name "Partnumber")
                (value "B4B-PH-SM4-TB(LF)(SN)")
            )
            (property
                (name "atopile_address")
                (value "uart_connector")
            )
            (tstamps "2")
            (fields)
        )
        (comp
            (ref "D1")
            (value "hongjiacheng_M1_package")
            (footprint "hongjiacheng_M1:SMA_L4.3-W2.6-LS5.0-RD")
            (property
                (name "LCSC")
                (value "C18199093")
            )
            (property
                (name "Manufacturer")
                (value "hongjiacheng")
            )
            (property
                (name "Partnumber")
                (value "M1")
            )
            (property
                (name "atopile_address")
                (value "power_protection_diode")
            )
            (tstamps "3")
            (fields)
        )
        (comp
            (ref "H1")
            (value "DFPlayer_Socket_Left")
            (footprint "hanxia_HX_PM2_54_1x8P_TP_H8_5_YQ:HDR-SMD_8P-P2.54-V-F-S4.7")
            (property
                (name "LCSC")
                (value "C46635844")
            )
            (property
                (name "Manufacturer")
                (value "hanxia")
            )
            (property
                (name "Partnumber")
                (value "HX PM2.54-1x8P TP H8.5-YQ")
            )
            (property
                (name "atopile_address")
                (value "df_header_left")
            )
            (tstamps "4")
            (fields)
        )
        (comp
            (ref "H2")
            (value "DFPlayer_Socket_Right")
            (footprint "hanxia_HX_PM2_54_1x8P_TP_H8_5_YQ:HDR-SMD_8P-P2.54-V-F-S4.7")
            (property
                (name "LCSC")
                (value "C46635844")
            )
            (property
                (name "Manufacturer")
                (value "hanxia")
            )
            (property
                (name "Partnumber")
                (value "HX PM2.54-1x8P TP H8.5-YQ")
            )
            (property
                (name "atopile_address")
                (value "df_header_right")
            )
            (tstamps "5")
            (fields)
        )
        (comp
            (ref "U1")
            (value "1kΩ ±1% 125mW")
            (footprint "UNI_ROYAL_0805W8F1001T5E:R0805")
            (property
                (name "LCSC")
                (value "C17513")
            )
            (property
                (name "Manufacturer")
                (value "UNI-ROYAL(Uniroyal Elec)")
            )
            (property
                (name "Partnumber")
                (value "0805W8F1001T5E")
            )
            (property
                (name "PARAM_max_power")
                (value "{\"type\": \"Quantity_Set_Discrete\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 0.125, \"max\": 0.125}}]}}, \"unit\": \"watt\"}}")
            )
            (property
                (name "PARAM_max_voltage")
                (value "{\"type\": \"Quantity_Set_Discrete\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 150.0, \"max\": 150.0}}]}}, \"unit\": \"volt\"}}")
            )
            (property
                (name "PARAM_resistance")
                (value "{\"type\": \"Quantity_Interval_Disjoint\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 990.0000002235174, \"max\": 1009.9999997764826}}]}}, \"unit\": \"ohm\"}}")
            )
            (property
                (name "atopile_address")
                (value "rx_protection_resistor")
            )
            (tstamps "6")
            (fields)
        )
        (comp
            (ref "U2")
            (value "JST_PH_Vertical_2Pin")
            (footprint "JST_Sales_America_B2B_PH_SM4_TBT_LF__SN:CONN-SMD_B2B-PH-SM4-TBT-LF-SN")
            (property
                (name "LCSC")
                (value "C265003")
            )
            (property
                (name "Manufacturer")
                (value "JST Sales America")
            )
            (property
                (name "Partnumber")
                (value "B2B-PH-SM4-TBT(LF)(SN)")
            )
            (property
                (name "atopile_address")
                (value "speaker_connector")
            )
            (tstamps "7")
            (fields)
        )
        (comp
            (ref "U3")
            (value "AudioJack3_5mm")
            (footprint "SOFNG_PJ_320B:AUDIO-SMD_PJ-320B")
            (property
                (name "LCSC")
                (value "C22355831")
            )
            (property
                (name "Manufacturer")
                (value "SOFNG")
            )
            (property
                (name "Partnumber")
                (value "PJ-320B")
            )
            (property
                (name "atopile_address")
                (value "stereo_out_jack")
            )
            (tstamps "8")
            (fields)
        )
    )
    (nets
        (net
            (code 1)
            (name "ADKEY_1")
            (node
                (ref "H2")
                (pin "4")
            )
        )
        (net
            (code 2)
            (name "ADKEY_2")
            (node
                (ref "H2")
                (pin "5")
            )
        )
        (net
            (code 3)
            (name "BUSY")
            (node
                (ref "H2")
                (pin "8")
            )
        )
        (net
            (code 4)
            (name "DAC_L")
            (node
                (ref "H1")
                (pin "5")
            )
            (node
                (ref "U3")
                (pin "1")
            )
        )
        (net
            (code 5)
            (name "DAC_R")
            (node
                (ref "H1")
                (pin "4")
            )
            (node
                (ref "U3")
                (pin "2")
            )
        )
        (net
            (code 6)
            (name "GND")
            (node
                (ref "C1")
                (pin "2")
            )
            (node
                (ref "CN1")
                (pin "2")
            )
            (node
                (ref "H1")
                (pin "7")
            )
            (node
                (ref "H2")
                (pin "2")
            )
            (node
                (ref "U3")
                (pin "3")
            )
        )
        (net
            (code 7)
            (name "IO_1")
            (node
                (ref "H2")
                (pin "1")
            )
        )
        (net
            (code 8)
            (name "IO_2")
            (node
                (ref "H2")
                (pin "3")
            )
        )
        (net
            (code 9)
            (name "K")
            (node
                (ref "C1")
                (pin "1")
            )
            (node
                (ref "D1")
                (pin "1")
            )
            (node
                (ref "H1")
                (pin "1")
            )
        )
        (net
            (code 10)
            (name "SPK_1")
            (node
                (ref "H1")
                (pin "6")
            )
            (node
                (ref "U2")
                (pin "1")
            )
        )
        (net
            (code 11)
            (name "SPK_2")
            (node
                (ref "H1")
                (pin "8")
            )
            (node
                (ref "U2")
                (pin "2")
            )
        )
        (net
            (code 12)
            (name "TX")
            (node
                (ref "CN1")
                (pin "4")
            )
            (node
                (ref "H1")
                (pin "3")
            )
        )
        (net
            (code 13)
            (name "USB_M")
            (node
                (ref "H2")
                (pin "7")
            )
        )
        (net
            (code 14)
            (name "USB_P")
            (node
                (ref "H2")
                (pin "6")
            )
        )
        (net
            (code 15)
            (name "VCC")
            (node
                (ref "CN1")
                (pin "1")
            )
            (node
                (ref "D1")
                (pin "2")
            )
        )
        (net
            (code 16)
            (name "_3")
            (node
                (ref "U2")
                (pin "3")
            )
        )
        (net
            (code 17)
            (name "_4")
            (node
                (ref "U2")
                (pin "4")
            )
        )
        (net
            (code 18)
            (name "_5")
            (node
                (ref "CN1")
                (pin "5")
            )
        )
        (net
            (code 19)
            (name "_6")
            (node
                (ref "CN1")
                (pin "6")
            )
        )
        (net
            (code 20)
            (name "df_header_left-RX")
            (node
                (ref "H1")
                (pin "2")
            )
            (node
                (ref "U1")
                (pin "2")
            )
        )
        (net
            (code 21)
            (name "footprint-RX")
            (node
                (ref "CN1")
                (pin "3")
            )
            (node
                (ref "U1")
                (pin "1")
            )
        )
        (net
            (code 22)
            (name "net")
            (node
                (ref "U3")
                (pin "")
            )
        )
    )
    (libparts)
    (libraries)
)