(kicad_pcb
    (version 20241229)
    (generator "pcbnew")
    (generator_version "9.0")
    (general
        (thickness 1.6)
        (legacy_teardrops no)
    )
    (paper "A4")
    (layers
        (0 "F.Cu" signal)
        (2 "B.Cu" signal)
        (9 "F.Adhes" user "F.Adhesive")
        (11 "B.Adhes" user "B.Adhesive")
        (13 "F.Paste" user)
        (15 "B.Paste" user)
        (5 "F.SilkS" user "F.Silkscreen")
        (7 "B.SilkS" user "B.Silkscreen")
        (1 "F.Mask" user)
        (3 "B.Mask" user)
        (17 "Dwgs.User" user "User.Drawings")
        (19 "Cmts.User" user "User.Comments")
        (21 "Eco1.User" user "User.Eco1")
        (23 "Eco2.User" user "User.Eco2")
        (25 "Edge.Cuts" user)
        (27 "Margin" user)
        (31 "F.CrtYd" user "F.Courtyard")
        (29 "B.CrtYd" user "B.Courtyard")
        (35 "F.Fab" user)
        (33 "B.Fab" user)
        (39 "User.1" user)
        (41 "User.2" user)
        (43 "User.3" user)
        (45 "User.4" user)
        (47 "User.5" user)
        (49 "User.6" user)
        (51 "User.7" user)
        (53 "User.8" user)
        (55 "User.9" user)
    )
    (setup
        (pad_to_mask_clearance 0)
        (allow_soldermask_bridges_in_footprints no)
        (tenting front back)
        (pcbplotparams
            (layerselection 0x00000000_00000000_000010fc_ffffffff)
            (plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
            (disableapertmacros no)
            (usegerberextensions no)
            (usegerberattributes yes)
            (usegerberadvancedattributes yes)
            (creategerberjobfile yes)
            (dashed_line_dash_ratio 12)
            (dashed_line_gap_ratio 3)
            (svgprecision 4)
            (plotframeref no)
            (mode 1)
            (useauxorigin no)
            (hpglpennumber 1)
            (hpglpenspeed 20)
            (hpglpendiameter 15)
            (pdf_front_fp_property_popups yes)
            (pdf_back_fp_property_popups yes)
            (pdf_metadata yes)
            (pdf_single_document no)
            (dxfpolygonmode yes)
            (dxfimperialunits yes)
            (dxfusepcbnewfont yes)
            (psnegative no)
            (psa4output no)
            (plot_black_and_white yes)
            (plotinvisibletext no)
            (sketchpadsonfab no)
            (plotreference yes)
            (plotvalue yes)
            (plotpadnumbers no)
            (hidednponfab no)
            (sketchdnponfab yes)
            (crossoutdnponfab yes)
            (plotfptext yes)
            (subtractmaskfromsilk no)
            (outputformat 1)
            (mirror no)
            (drillshape 1)
            (scaleselection 1)
            (outputdirectory "")
        )
    )
    (net 0 "")
    (net 1 "footprint-_4")
    (net 2 "df_header_right-_5")
    (net 3 "footprint-_6")
    (net 4 "df_header_right-_4")
    (net 5 "df_header_right-_2")
    (net 6 "footprint-_3-1")
    (net 7 "footprint-_5")
    (net 8 "df_header_right-_3")
    (net 9 "df_header_right-_1")
    (net 10 "df_header_left-_2-1")
    (net 11 "gnd")
    (net 12 "df_header_left-_1")
    (net 13 "v_in_5v")
    (net 15 "RING")
    (net 16 "v_dfplayer")
    (net 17 "df_header_left-_3")
    (net 18 "_7")
    (net 19 "TIP")
    (net 20 "df_header_right-_6")
    (net 21 "net")
    (net 22 "df_header_left-_2-0")
    (net 23 "footprint-_3-0")
    (footprint "hanxia_HX_PM2_54_1x8P_TP_H8_5_ZQ:HDR-SMD_8P-P2.54-V-F-LS4.7"
        (layer "F.Cu")
        (uuid "38438bc1-0725-420f-860a-49df4642524b")
        (at 152.61 81 0)
        (property "Reference" "H2"
            (at 0.89 -3.5 0)
            (layer "F.SilkS")
            (hide no)
            (uuid "1394c5fc-6b36-4b57-8860-2f1260f5f5df")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 0 5.5 0)
            (layer "F.Fab")
            (hide no)
            (uuid "46786dfe-bc98-4e7b-9e30-aaacdec17ac7")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 0)
            (layer "F.Fab")
            (hide yes)
            (uuid "337cfa8b-b12f-42bb-8917-ffe2fe5fa596")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 0)
            (layer "F.Fab")
            (hide yes)
            (uuid "44262d5b-19f0-4754-87a8-3f51d415e07d")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "e1ae12f555519af8c11439d0a2175ddbbdd080e821244f82aff68eb0bebf1f55"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "c57eb9dc-59b1-4c0a-a46a-ca4b82054a05")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "__atopile_lib_fp_hash__" "0eae38e2-f249-5e39-dd2b-1da477ebfd1d"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "9bbaac35-06c8-42f6-aaa9-c4034642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C48641756"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "514359c8-bddd-4d05-b8bb-4b834642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "hanxia"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "3c910c64-e63b-4483-903d-96b44642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "HX PM2.54-1x8P TP H8.5-ZQ"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "14e5693e-8766-42b8-8f0e-0f124642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "df_header_right"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "91fc8df5-70d8-49a9-935b-cb744642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -10.16 -1.27)
            (end -7.22 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "27c25baa-07a8-47ab-aed3-e529f8cfd94e")
        )
        (fp_line
            (start -10.16 1.27)
            (end -10.16 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "47928c4a-211d-4747-945c-7daba51e6793")
        )
        (fp_line
            (start -9.75 1.27)
            (end -10.16 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "1a50656e-5150-46b9-9041-a149d94eae6a")
        )
        (fp_line
            (start -5.49 -1.27)
            (end -2.13 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "86e6116e-c1ef-416d-96b8-bcddaf7c9e52")
        )
        (fp_line
            (start -4.67 1.27)
            (end -8.02 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "67904f8f-5d41-4cb1-a6f8-672ed31c7661")
        )
        (fp_line
            (start -0.4 -1.27)
            (end 2.95 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "b56eda59-25b6-4026-8ee6-2f012a1733f2")
        )
        (fp_line
            (start 0.4 1.27)
            (end -2.95 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "47735969-4d23-4b02-a8e6-e73204a3210f")
        )
        (fp_line
            (start 4.67 -1.27)
            (end 8.02 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "542c3745-ca0f-4d04-949c-72e8ee4975e6")
        )
        (fp_line
            (start 5.49 1.27)
            (end 2.13 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "adf106dc-4bb7-41fb-bf80-1d279cb93e85")
        )
        (fp_line
            (start 7.22 1.27)
            (end 10.15 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "23edc440-3767-4ca3-afd7-8f2170c934a8")
        )
        (fp_line
            (start 10.15 -1.27)
            (end 9.75 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "0291117d-4b27-40cd-8c79-afa333cf09b2")
        )
        (fp_line
            (start 10.15 -1.27)
            (end 10.15 -0.51)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "08dcac5a-5751-42b8-8069-aff6f0fa6a4c")
        )
        (fp_line
            (start 10.15 -0.51)
            (end 10.15 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "45996e11-a110-4fcc-a27e-bb51009508e1")
        )
        (fp_circle
            (center -10.16 2.54)
            (end -10.01 2.54)
            (stroke
                (width 0.3)
                (type solid)
            )
            (fill no)
            (layer "F.SilkS")
            (uuid "03d2b660-52d6-44dc-8641-73779a777df0")
        )
        (fp_circle
            (center -10.16 2.4)
            (end -10.13 2.4)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "50e83014-8d93-48e3-aff8-3088e9333086")
        )
        (fp_text user "${REFERENCE}"
            (at 0 0 0)
            (layer "F.Fab")
            (uuid "d29ec92a-b986-49f7-93aa-ab1ba5697472")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at -8.89 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 9 "df_header_right-_1")
            (uuid "43e0937e-042f-4adf-860d-6e960e1e3e53")
        )
        (pad "2" smd rect
            (at -6.35 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 5 "df_header_right-_2")
            (uuid "c44cd2a0-1565-43da-828a-f9c65c433e61")
        )
        (pad "3" smd rect
            (at -3.81 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 8 "df_header_right-_3")
            (uuid "63a44832-9667-4671-b2ea-e1fde9c6e5d8")
        )
        (pad "4" smd rect
            (at -1.27 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 4 "df_header_right-_4")
            (uuid "585485a1-881e-42a1-8342-c0a66dff7b0b")
        )
        (pad "5" smd rect
            (at 1.27 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 2 "df_header_right-_5")
            (uuid "c543f00f-b2e2-4da8-aded-b786783994b9")
        )
        (pad "6" smd rect
            (at 3.81 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 20 "df_header_right-_6")
            (uuid "48d277da-3e76-4991-bdc8-969346636169")
        )
        (pad "7" smd rect
            (at 6.35 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 18 "_7")
            (uuid "5a3c3944-e722-482e-bf30-fc455e275b52")
        )
        (pad "8" smd rect
            (at 8.89 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 11 "gnd")
            (uuid "be175495-a7f5-4746-ab23-541efe468cab")
        )
        (embedded_fonts no)
    )
    (footprint "JST_Sales_America_B4B_PH_SM4_TB_LF__SN:CONN-SMD_B4B-PH-SM4-TB-LF-SN"
        (layer "F.Cu")
        (uuid "4719d4be-d6db-4088-b95a-d1624642524b")
        (at 134.66 88.35 -90)
        (property "Reference" "CN1"
            (at 0 -5.16 90)
            (layer "F.SilkS")
            (hide no)
            (uuid "b35da03a-13d0-4f4a-855a-dd648fa0cbd3")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 0 5.16 90)
            (layer "F.Fab")
            (hide no)
            (uuid "ebe96335-a6ca-40cb-90b7-2d9b91ff1667")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "dd628ff0-b608-488b-b987-613a699ef7ad")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "025f6d40-93cc-451c-b293-f7df4786e55b")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "3d5236078eef95c9994de747335534563e82e3ec7a20c14f1274c15f5ec98bab"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "eaef3bb7-58cb-4d58-8f2e-d5b3d76e5df6")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "__atopile_lib_fp_hash__" "cc27e38c-cc5b-e0b4-993a-7b2b9b9f0b24"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "1c4cb747-1faf-4d9f-b7ec-c6db4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C160354"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "8f09155a-b6f8-4e76-ab66-f50f4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "JST Sales America"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "ad7c7dcf-c8c4-4a3e-b838-be454642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "B4B-PH-SM4-TB(LF)(SN)"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "7c4b90f6-2f4c-42bc-ad4e-215e4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "uart_connector"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "1fb844d7-c01e-4aee-9904-4af14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -6 3.67)
            (end -6 3.09)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "51bab4b8-bb12-40be-9cd6-97f000ebaf93")
        )
        (fp_line
            (start 6 3.67)
            (end -6 3.67)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "e5e71195-818d-4479-9d6c-59e44151dadc")
        )
        (fp_line
            (start 6 3.09)
            (end 6 3.67)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "c06966ac-cf7b-4a84-95f0-efa0cbc98234")
        )
        (fp_line
            (start -6 -1.33)
            (end -6 -0.77)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "597d1fd2-536f-42d7-9fb4-61235f8a612a")
        )
        (fp_line
            (start -6 -1.33)
            (end -4 -1.33)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "97d3679a-4dec-4290-8582-65925f0df611")
        )
        (fp_line
            (start 4 -1.33)
            (end 6 -1.33)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "150d604e-5c55-4729-984e-1ba4f7d9324c")
        )
        (fp_line
            (start 6 -1.33)
            (end 6 -0.77)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "c71e4c02-903b-49ce-830e-fe7ac24d6215")
        )
        (fp_circle
            (center 5.98 -3.33)
            (end 6.01 -3.33)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "89729549-ec78-47e0-b3ac-efb59cf5b9da")
        )
        (fp_text user "${REFERENCE}"
            (at 0 -5.16 90)
            (layer "F.SilkS")
            (uuid "1d5c9585-2fc0-483e-88c0-b5b2da278364")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 0 90)
            (layer "F.Fab")
            (uuid "44180ab9-f906-409a-9532-86bcb9ace589")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at 3 -1.16 90)
            (size 1 6)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 13 "v_in_5v")
            (uuid "33508cea-4d77-4e4d-815d-d83e66575bb3")
        )
        (pad "2" smd rect
            (at 1 -1.16 90)
            (size 1 6)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 11 "gnd")
            (uuid "5800a866-184b-424e-95e4-619545072273")
        )
        (pad "3" smd rect
            (at -1 -1.16 90)
            (size 1 6)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 23 "footprint-_3-0")
            (uuid "23fad4d9-9574-4357-9d8b-64857a50cf3f")
        )
        (pad "4" smd rect
            (at -3 -1.16 90)
            (size 1 6)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 17 "df_header_left-_3")
            (uuid "65e50188-d0df-4e07-a74f-4a9640625694")
        )
        (pad "5" smd rect
            (at -5.35 1.16 270)
            (size 1.8 3.4)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 7 "footprint-_5")
            (uuid "57b0c870-c382-46ae-be03-517313769f8c")
        )
        (pad "6" smd rect
            (at 5.35 1.16 270)
            (size 1.8 3.4)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 3 "footprint-_6")
            (uuid "74a89d37-3e6d-4142-82a1-5edf56ec309d")
        )
        (embedded_fonts no)
        (model "${KIPRJMOD}/../../parts/JST_Sales_America_B4B_PH_SM4_TB_LF__SN/CONN-SMD_B4B-PH-SM4-TBT-LF-SN.step"
            (offset
                (xyz 0 0 0)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 180)
            )
        )
    )
    (footprint "hongjiacheng_M1:SMA_L4.3-W2.6-LS5.0-RD"
        (layer "F.Cu")
        (uuid "84844f8d-27ff-41d9-b638-27474642524b")
        (at 136.5 101 90)
        (property "Reference" "D1"
            (at 0 -4.01 90)
            (layer "F.SilkS")
            (hide no)
            (uuid "bdc6be2b-82df-4feb-8f34-eeda91569bb3")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 71.15 88.01 90)
            (layer "F.Fab")
            (hide no)
            (uuid "470cbdac-ff56-412b-bf37-3adff77dcca4")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "24414e52-d495-4426-bb7a-15f63da96bb8")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "7bebc76f-10f2-45db-9c05-31242a3a2fe3")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "2dfdc9ed9d9466ae17a15c91565d76685b0c8ccff8af20b86f22d63b5da996ce"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "e553dd8a-978a-43df-8e9f-acc257d4920a")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "__atopile_lib_fp_hash__" "f03d4610-e43b-4332-0c10-ee29038f0dcb"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "8c97c7b3-f113-42d5-91cc-2dfa4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C18199093"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "a325d6ed-2c56-4626-ba9e-414f4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "hongjiacheng"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "e75f0411-50f6-4ac9-9679-b77e4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "M1"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "74a0a020-3b81-4d92-9423-9a194642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "power_protection_diode"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "c96116cc-7333-4807-a854-eb544642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -1.08 -1.36)
            (end -1.08 1.36)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "7243c809-6155-4697-904a-a84e748f0477")
        )
        (fp_line
            (start -2.53 -1.36)
            (end 2.16 -1.35)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "9d69c972-7a7b-407c-9c89-f7bbffe6d5a4")
        )
        (fp_line
            (start 2.16 -1.27)
            (end 2.16 -0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "ce18a7a8-2848-4dee-b035-9f32365d9ec0")
        )
        (fp_line
            (start 2.16 1.36)
            (end 2.16 1.01)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "2f0e635e-4ca9-4c7b-962e-4a7e41a06042")
        )
        (fp_line
            (start -2.5 1.36)
            (end 2.16 1.36)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "967291e9-6d4d-48c2-8922-83e523db2491")
        )
        (fp_circle
            (center -2.5 1.3)
            (end -2.47 1.3)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "1c5f787c-1a37-4a2d-a820-8829cf6d6ac2")
        )
        (fp_text user "${REFERENCE}"
            (at 0 -4.01 90)
            (layer "F.SilkS")
            (uuid "fe43e9f2-3a46-48ab-ab29-6f2004d4113e")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 0 90)
            (layer "F.Fab")
            (uuid "69d3cace-c0d5-4073-87a3-d73afeb09b60")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at -2.4 0.01 90)
            (size 2.05 1.62)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 16 "v_dfplayer")
            (uuid "eca840e3-1a6d-4200-ad49-ca56d2ccfe4c")
        )
        (pad "2" smd rect
            (at 2.4 -0.01 270)
            (size 2.05 1.62)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 13 "v_in_5v")
            (uuid "2221c711-ef8c-43f0-935d-d662c1165436")
        )
        (embedded_fonts no)
        (model "${KIPRJMOD}/../../parts/hongjiacheng_M1/SMA_L4.3-W2.6-LS5.0-RD.STEP"
            (offset
                (xyz 0 0 0)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 0)
            )
        )
    )
    (footprint "UNI_ROYAL_0805W8F1001T5E:R0805"
        (layer "F.Cu")
        (uuid "86526136-778c-448a-99dd-4c0a4642524b")
        (at 146.43 88 0)
        (property "Reference" "U1"
            (at 0 -4 0)
            (layer "F.SilkS")
            (hide no)
            (uuid "1b95590f-7aee-45da-b3a5-d6c38a81d2dc")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" "1kΩ ±1% 125mW"
            (at 0 4 0)
            (layer "F.Fab")
            (hide no)
            (uuid "589dd85a-79e4-42f8-8aff-1785c0f20f54")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311800_UNI-ROYAL-Uniroyal-Elec-0805W8F1001T5E_C17513.pdf"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "7f2070f5-763c-4a14-982a-ec6b45d6f2cd")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Description" ""
            (at 0 0 0)
            (layer "F.Fab")
            (hide yes)
            (uuid "d5286a5b-24a5-41e1-9810-2fe569952aa6")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "3be0a787d4424e3a01f0ee8aa3acb6b2ae7ef35b340ce15481d10ca9f3373768"
            (at 0 0 0)
            (layer "User.9")
            (hide no)
            (uuid "d3554747-903f-49d3-b458-e7f5f765b0d8")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
                (hide yes)
            )
        )
        (property "__atopile_lib_fp_hash__" "e44d99a9-7851-0af8-7a57-5bfc4424bb89"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "99509816-0097-4152-a110-67704642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C17513"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "8dfafb68-f9c8-47a7-a044-a3364642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "UNI-ROYAL(Uniroyal Elec)"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "66dbe0f7-c1ba-4739-b483-8e9b4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "0805W8F1001T5E"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "f64925e6-00c4-4265-8966-93d54642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "PARAM_max_power" "{\"type\": \"Quantity_Set_Discrete\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 0.125, \"max\": 0.125}}]}}, \"unit\": \"watt\"}}"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "334d3f65-dc11-4ae7-a629-d0d14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "PARAM_max_voltage" "{\"type\": \"Quantity_Set_Discrete\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 150.0, \"max\": 150.0}}]}}, \"unit\": \"volt\"}}"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "08bc7d1b-40b8-468e-ba9f-fe664642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "PARAM_resistance" "{\"type\": \"Quantity_Interval_Disjoint\", \"data\": {\"intervals\": {\"type\": \"Numeric_Interval_Disjoint\", \"data\": {\"intervals\": [{\"type\": \"Numeric_Interval\", \"data\": {\"min\": 990.0000002235174, \"max\": 1009.9999997764826}}]}}, \"unit\": \"ohm\"}}"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "a6445313-87bd-4bb5-9cd8-b3f14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "rx_protection_resistor"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "7d6c984d-49bc-461b-8a04-ac984642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start 0.48 0.92)
            (end 1.76 0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "d9d5248a-b2bd-4340-b6f3-abcc084d50f1")
        )
        (fp_line
            (start 1.76 0.92)
            (end 1.76 -0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "291d0000-fc48-4e34-b808-a0af6c2c87bb")
        )
        (fp_line
            (start 1.76 -0.92)
            (end 0.48 -0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "64ac47fd-4f35-4e15-a8ea-d3321e20c99d")
        )
        (fp_line
            (start -0.48 0.92)
            (end -1.76 0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "288cc0f1-e62f-48e3-9ce0-8c58d148080f")
        )
        (fp_line
            (start -1.76 0.92)
            (end -1.76 -0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "50bf3c50-4feb-47bf-8427-0f5741f1a6cf")
        )
        (fp_line
            (start -1.76 -0.92)
            (end -0.48 -0.92)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "ba4f08b5-2e35-40a9-bd7b-049cda409bb4")
        )
        (fp_circle
            (center -1 0.64)
            (end -0.97 0.64)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "b5fa2cc5-6525-4907-bb60-d76af14ce64f")
        )
        (fp_text user "%R"
            (at 0 0 0)
            (layer "F.Fab")
            (uuid "bba02050-dab4-4423-82b9-b2b5ceea683c")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 -4 0)
            (layer "F.SilkS")
            (uuid "1b95590f-7aee-45da-b3a5-d6c38a81d2dc")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "2" smd rect
            (at 1 0 0)
            (size 1.13 1.38)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 22 "df_header_left-_2-0")
            (uuid "3752a4f8-b6bb-4177-aaa9-19e5ec10d32c")
        )
        (pad "1" smd rect
            (at -1 0 0)
            (size 1.13 1.38)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 23 "footprint-_3-0")
            (uuid "ae7bde01-25db-4b24-bb9a-9b8bc594c5b0")
        )
        (model "${KIPRJMOD}/../../parts/UNI_ROYAL_0805W8F1001T5E/R0805_L2.0-W1.3-H0.6.step"
            (offset
                (xyz 0 0 0)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 0)
            )
        )
    )
    (footprint "hanxia_HX_PM2_54_1x8P_TP_H8_5_ZQ:HDR-SMD_8P-P2.54-V-F-LS4.7"
        (layer "F.Cu")
        (uuid "bfe8ac0a-d3cd-4e7c-9a0f-6ff64642524b")
        (at 153.11 102.5 0)
        (property "Reference" "H1"
            (at 0 -5.5 0)
            (layer "F.SilkS")
            (hide no)
            (uuid "e1fdcb25-bbb7-480b-a3eb-ca2182d4a17c")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 0 5.5 0)
            (layer "F.Fab")
            (hide no)
            (uuid "e6735211-f1b3-4a8d-a8a6-ddd8d9cce98f")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 0)
            (layer "F.Fab")
            (hide yes)
            (uuid "b609117e-058c-4c2e-a923-ab17bf02f4dd")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 0)
            (layer "F.Fab")
            (hide yes)
            (uuid "34c3213a-e7b2-4932-945d-3a84597506b1")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "e1ae12f555519af8c11439d0a2175ddbbdd080e821244f82aff68eb0bebf1f55"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "c57eb9dc-59b1-4c0a-a46a-ca4b82054a05")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "__atopile_lib_fp_hash__" "0eae38e2-f249-5e39-dd2b-1da477ebfd1d"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "6e61aa35-c501-45e5-8d08-1b7e4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C48641756"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "47dfa67e-ed26-42a1-9f05-26774642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "hanxia"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "00f59694-8ebe-4b4f-a19f-c83b4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "HX PM2.54-1x8P TP H8.5-ZQ"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "89e98553-d3d0-479b-8ff0-64114642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "df_header_left"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "c0bd2da2-48d8-49e5-a9c5-66084642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -10.16 -1.27)
            (end -7.22 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "a3d6dfd4-6734-4927-a957-05e3dc6140ce")
        )
        (fp_line
            (start -10.16 1.27)
            (end -10.16 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "1bd1ae5a-0142-45fa-a407-9206686723ba")
        )
        (fp_line
            (start -9.75 1.27)
            (end -10.16 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "0614385d-9bf9-4ef3-82b6-a83d514d87c4")
        )
        (fp_line
            (start -5.49 -1.27)
            (end -2.13 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "7a1d7a0e-7ce5-46b1-aeb4-0c8fdc0b5e5d")
        )
        (fp_line
            (start -4.67 1.27)
            (end -8.02 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "9664ed60-714e-4f63-960a-b936fc4647d3")
        )
        (fp_line
            (start -0.4 -1.27)
            (end 2.95 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "219acf0c-bff7-4e14-9c0d-4aa72300865e")
        )
        (fp_line
            (start 0.4 1.27)
            (end -2.95 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "6a3c726a-a4fb-4db1-9faf-10daa681229f")
        )
        (fp_line
            (start 4.67 -1.27)
            (end 8.02 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "88260e44-03bb-472a-b0b7-bfc980f8a560")
        )
        (fp_line
            (start 5.49 1.27)
            (end 2.13 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "92270ee3-3b03-4d15-89cc-25d42e1a68f2")
        )
        (fp_line
            (start 7.22 1.27)
            (end 10.15 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "e2696bdc-e1af-410c-bf01-70efd20c9991")
        )
        (fp_line
            (start 10.15 -1.27)
            (end 9.75 -1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "9fe7b994-fabf-4967-ba95-ba1ef22ac473")
        )
        (fp_line
            (start 10.15 -1.27)
            (end 10.15 -0.51)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "bd068a07-dcf1-4279-82e5-2be285c6b171")
        )
        (fp_line
            (start 10.15 -0.51)
            (end 10.15 1.27)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "3041c736-cad2-4538-a405-217b0583e46d")
        )
        (fp_circle
            (center -10.16 2.54)
            (end -10.01 2.54)
            (stroke
                (width 0.3)
                (type solid)
            )
            (fill no)
            (layer "F.SilkS")
            (uuid "57cc6a1d-bd3d-43bb-bd86-97116c66cfd0")
        )
        (fp_circle
            (center -10.16 2.4)
            (end -10.13 2.4)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "9f95cfa0-d1bd-4315-9a64-26c9896bacbd")
        )
        (fp_text user "${REFERENCE}"
            (at 0 -5.5 0)
            (layer "F.SilkS")
            (uuid "22e6a931-c2c4-412d-a27b-dfb98dca363a")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 0 0)
            (layer "F.Fab")
            (uuid "aa94f2c5-ea48-45ac-abb9-17c29da40240")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at -8.89 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 16 "v_dfplayer")
            (uuid "0b4a9f64-89fe-4b66-af32-c2df7be08c09")
        )
        (pad "2" smd rect
            (at -6.35 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 22 "df_header_left-_2-0")
            (uuid "5094a899-3132-4fb1-92b2-b23f8a7f1ac2")
        )
        (pad "3" smd rect
            (at -3.81 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 17 "df_header_left-_3")
            (uuid "418d2820-79dd-4774-89ec-5e1cc2077416")
        )
        (pad "4" smd rect
            (at -1.27 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 19 "TIP")
            (uuid "ce158f8c-ef79-4474-bb57-93b0ae7cd8e2")
        )
        (pad "5" smd rect
            (at 1.27 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 15 "RING")
            (uuid "5d145eb8-cce2-4595-a38a-b1acf7fe4c95")
        )
        (pad "6" smd rect
            (at 3.81 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 12 "df_header_left-_1")
            (uuid "37c4b44f-eb20-43a8-ac8a-94d7ec55b7cd")
        )
        (pad "7" smd rect
            (at 6.35 1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 10 "df_header_left-_2-1")
            (uuid "46c85612-6230-4434-b26f-8fbad3d5b776")
        )
        (pad "8" smd rect
            (at 8.89 -1.5 180)
            (size 1.02 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 11 "gnd")
            (uuid "30e38b82-4508-4f5d-bdee-a1985b0077eb")
        )
        (embedded_fonts no)
    )
    (footprint "JST_Sales_America_B2B_PH_SM4_TBT_LF__SN:CONN-SMD_B2B-PH-SM4-TBT-LF-SN"
        (layer "F.Cu")
        (uuid "e269d19c-fbbb-488c-9967-b9724642524b")
        (at 167.38 90 -90)
        (property "Reference" "U2"
            (at 0 -5.12 90)
            (layer "F.SilkS")
            (hide no)
            (uuid "f1c6fd17-f458-4b60-8df5-00e09e398f8c")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 0 5.12 90)
            (layer "F.Fab")
            (hide no)
            (uuid "53bcdd7e-3c13-4525-a7c4-44fa41b63003")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "2ae2437a-3b26-43c1-88e7-be09ec4064ad")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "4fbb94ef-ec5c-4f2f-8883-78491d993a3b")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "2d56ab1e5cd62f070d2f25da6a505ce39581397fbebb96f028b8479d86a2656b"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "1db36e15-f4b1-4b5e-9d26-8669a71f3365")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "__atopile_lib_fp_hash__" "469f518d-33f9-4b2f-3288-c12ae864894f"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "b95b7551-484b-4e73-b0fb-d4b04642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C265003"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "b0f4c40c-ca31-4223-918e-875c4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "JST Sales America"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "7bff1645-df9a-4129-9175-a0ed4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "B2B-PH-SM4-TBT(LF)(SN)"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "b0557ce6-9ad3-4285-b8e9-702d4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "speaker_connector"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "83e26928-efcc-4e39-a0df-0a014642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -4 1.37)
            (end -1.73 1.37)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "c0b22978-fd80-4fd5-bdc3-7a62f9c71684")
        )
        (fp_line
            (start -0.27 1.37)
            (end 0.27 1.37)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "822fe15c-15a9-488c-bbf3-0e384e836f8b")
        )
        (fp_line
            (start 1.73 1.37)
            (end 4 1.37)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "bbb530c7-462d-42c8-ad26-cb6ff786b863")
        )
        (fp_line
            (start 4 1.37)
            (end 4 0.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "fcfe6d36-2516-4eb8-9caf-c55c43212090")
        )
        (fp_line
            (start -4 0.6)
            (end -4 1.37)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "94d03034-fbdc-47a4-a7bc-aaf06a4c889f")
        )
        (fp_line
            (start 4 -2.86)
            (end 4 -3.63)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "d0b4f0db-64a2-4893-be7b-e0417c3c0dd3")
        )
        (fp_line
            (start -4 -3.63)
            (end -4 -2.86)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "72e9119c-8ca6-434b-96d2-3d5731f876ba")
        )
        (fp_line
            (start -4 -3.63)
            (end 4 -3.63)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "30641db5-9964-4671-855a-0d94cf1be66a")
        )
        (fp_circle
            (center -0.95 3.07)
            (end -0.82 3.07)
            (stroke
                (width 0.25)
                (type solid)
            )
            (fill no)
            (layer "Cmts.User")
            (uuid "ce18044f-e079-4527-a32c-9f78b1eed09a")
        )
        (fp_circle
            (center -3.97 3.38)
            (end -3.94 3.38)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "b19e2870-65e6-443e-8c84-899299d4b156")
        )
        (fp_text user "${REFERENCE}"
            (at 0 -5.12 90)
            (layer "F.SilkS")
            (uuid "079caf58-84f3-44c7-a8ba-362aeb5f16f8")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 0 90)
            (layer "F.Fab")
            (uuid "ae17cc2e-b204-4a94-be5f-e57ca9558c51")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at -1 1.12 270)
            (size 1 5.5)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 12 "df_header_left-_1")
            (uuid "c16bb4aa-8ef7-432f-a49d-c6c32f5391e5")
        )
        (pad "2" smd rect
            (at 1 1.12 270)
            (size 1 5.5)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 10 "df_header_left-_2-1")
            (uuid "ad5511c4-fa78-461e-964e-9de6eea69c99")
        )
        (pad "3" smd rect
            (at 3.5 -1.12 270)
            (size 2 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 6 "footprint-_3-1")
            (uuid "7474c68e-8312-415f-bf65-71ed1771361d")
        )
        (pad "4" smd rect
            (at -3.5 -1.12 270)
            (size 2 3)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 1 "footprint-_4")
            (uuid "648ef6f5-05e3-43fd-bd06-98078cc639fc")
        )
        (embedded_fonts no)
        (model "${KIPRJMOD}/../../parts/JST_Sales_America_B2B_PH_SM4_TBT_LF__SN/CONN-SMD_B2B-PH-SM4-TBT-LF-SN.step"
            (offset
                (xyz 0 0 0)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 0)
            )
        )
    )
    (footprint "PANASONIC_EEEFK1A471AP:CAP-SMD_BD8.0-L8.3-W8.3-LS9.9-FD"
        (layer "F.Cu")
        (uuid "e9d09963-cdb6-4e5d-8574-ee494642524b")
        (at 144.6 114.5 -90)
        (property "Reference" "C1"
            (at 0 -4 90)
            (layer "F.SilkS")
            (hide no)
            (uuid "623ea059-aff4-4353-aaf8-8b5f597349bf")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 0 4 90)
            (layer "F.Fab")
            (hide no)
            (uuid "edd08b58-caf8-4cc1-afc3-307a4b958dbe")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "a7b3b065-3cec-443d-a3d4-b1844759c7d9")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "5cfa12c7-d1ba-444d-8e59-225d285ff1a1")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "3a30aba91912392ddab4b95cf4c5624802b3c2048a8d62eb75165e8d2cddd84a"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "8c3ea71c-3b17-46b5-8887-cde37fc138d0")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "__atopile_lib_fp_hash__" "e27c02ec-f5a4-b701-e77f-3b41c05f2ff7"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "b4daf2ab-5f59-458c-8889-cda44642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C178529"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "a2b2130e-d6f2-47a0-a97c-b84a4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "PANASONIC"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "49b5c3db-d442-410a-a8af-c9814642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "EEEFK1A471AP"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "3a4898c1-fe60-4fdc-8db1-af654642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "power_filter_cap"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "7cbfb758-8aa2-4990-b182-08a14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -2.46 4.23)
            (end -4.2 2.49)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "e6798260-0ce2-41f1-b2f3-9e99838a29a4")
        )
        (fp_line
            (start 4.2 4.23)
            (end -2.46 4.23)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "ee682e10-4e8e-4ece-ba53-ae3d8778abaa")
        )
        (fp_line
            (start -4.2 2.49)
            (end -4.2 0.78)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "2c977140-e2a0-480f-b30a-b9d26b6986aa")
        )
        (fp_line
            (start 4.2 0.78)
            (end 4.2 4.23)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "7d872c1b-d9e7-49dc-92ab-9bcae2358fff")
        )
        (fp_line
            (start 4.2 -0.78)
            (end 4.2 -4.23)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "7b182ed0-6e93-48b4-8e41-e144aa20b298")
        )
        (fp_line
            (start -4.2 -2.49)
            (end -4.2 -0.78)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "94991dbb-c964-4563-99e5-af6404401655")
        )
        (fp_line
            (start -2.46 -4.23)
            (end -4.2 -2.49)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "339f79a3-2602-4119-804e-f418a9ad5670")
        )
        (fp_line
            (start 4.2 -4.23)
            (end -2.46 -4.23)
            (stroke
                (width 0.15)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "ab041e32-8109-4b1c-b56b-32d3e8d87c2e")
        )
        (fp_circle
            (center -4.95 4.15)
            (end -4.92 4.15)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "93fb89ed-b399-4512-b84a-c132e4b74c7a")
        )
        (fp_text user "${REFERENCE}"
            (at 0 -4 90)
            (layer "F.SilkS")
            (uuid "bb1962e4-04e1-4cf6-903e-94a76039cf3e")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 0 90)
            (layer "F.Fab")
            (uuid "fab31861-4a29-436f-acfb-d057f1eedb26")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at -3.6 0 270)
            (size 4.3 1.26)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 16 "v_dfplayer")
            (uuid "3aa34514-5a54-4e7d-8ebd-6078bca838b8")
        )
        (pad "2" smd rect
            (at 3.6 0 270)
            (size 4.3 1.26)
            (layers "F.Cu" "F.Mask" "F.Paste")
            (net 11 "gnd")
            (uuid "91f18ca7-ce55-4fd0-b3cc-a3af30352a21")
        )
        (embedded_fonts no)
        (model "${KIPRJMOD}/../../parts/PANASONIC_EEEFK1A471AP/CAP-SMD_BD8.0-L8.3-W8.3-LS9.9-FD.step"
            (offset
                (xyz 0 0 0)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 180)
            )
        )
    )
    (footprint "SOFNG_PJ_320B:AUDIO-SMD_PJ-320B"
        (layer "F.Cu")
        (uuid "f0eb9a9f-2671-4b53-8da2-f6cd4642524b")
        (at 156.3 116.8 -90)
        (property "Reference" "U3"
            (at 0 -7.5 0)
            (layer "F.SilkS")
            (hide no)
            (uuid "be499d2b-ceff-42c4-ae9f-e0cf276282c3")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Value" ""
            (at 0 7.5 0)
            (layer "F.Fab")
            (hide no)
            (uuid "dc5db5a9-a1f7-42df-ab7f-aff4f953b13d")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
        )
        (property "Datasheet" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "1facdcc8-14fb-416f-a87d-0acba5215f2f")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "Description" ""
            (at 0 0 90)
            (layer "F.Fab")
            (hide yes)
            (uuid "488037d5-4e9d-413a-8ace-a5f8ba25ee40")
            (effects
                (font
                    (size 1.27 1.27)
                    (thickness 0.15)
                )
            )
        )
        (property "checksum" "985abb5c5ae306cde70e644fc7a519056db632b07114d61a7ce01ffd2efb0f20"
            (at 0 0 0)
            (layer "User.9")
            (hide no)
            (uuid "62af287f-ee27-43c3-b5c5-76d8ba513648")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
                (hide yes)
            )
        )
        (property "__atopile_lib_fp_hash__" "bcd0fdc4-d6f3-489f-d358-90318b452c1d"
            (at 0 0 0)
            (layer "User.9")
            (hide yes)
            (uuid "b6f15f24-02b3-4f08-9185-ce024642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "LCSC" "C22355831"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "e2e3b294-9af2-4ef5-a651-9cbe4642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Manufacturer" "SOFNG"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "45c4b926-b0c3-408c-9957-25174642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "Partnumber" "PJ-320B"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "c5360e15-d098-4ee4-b08f-95434642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (property "atopile_address" "stereo_out_jack"
            (at 0 0 90)
            (layer "User.9")
            (hide yes)
            (uuid "4d10404e-cb83-41cc-a8c2-13b14642524b")
            (effects
                (font
                    (size 0.125 0.125)
                    (thickness 0.01875)
                )
            )
        )
        (attr smd)
        (fp_line
            (start -3 -5.6)
            (end 3 -5.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "84248522-c4c8-44ef-bce2-3232672fca83")
        )
        (fp_line
            (start 3 5.4)
            (end -3 5.4)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "b6f9dfac-df11-449e-9984-ba472b91b69d")
        )
        (fp_line
            (start -2.5 -5.6)
            (end -2.5 -8.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "2ab5d2b9-b593-41b7-ba1e-e8bddb1cdc55")
        )
        (fp_line
            (start -2.5 -8.6)
            (end 2.5 -8.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "3c991bb5-e6f6-4fbe-81d0-a8a1304b224a")
        )
        (fp_line
            (start 2.5 -5.6)
            (end 2.5 -8.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "58fae45d-82d6-4f47-8283-8a338d54815b")
        )
        (fp_line
            (start 3 3.4)
            (end 2.3 3.4)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "c44a98ba-c637-46b3-8349-b7ab4c73ac34")
        )
        (fp_line
            (start 2.3 3.4)
            (end 2.3 4.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "1a67b0d7-8d92-42b7-8ad5-e9083258ece1")
        )
        (fp_line
            (start 2.3 4.6)
            (end 3 4.6)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "01d86d62-72e1-44c9-b0ba-64c53c7c5bde")
        )
        (fp_line
            (start 3 4.6)
            (end 3 5.4)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "13bd1d5a-7877-4165-8a30-6e8f656248d1")
        )
        (fp_line
            (start -3 -5.6)
            (end -3 -4.48)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "d5753a7b-184c-4f0f-ba0f-de057b658fa1")
        )
        (fp_line
            (start -3 -2.52)
            (end -3 2.52)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "fcddfa29-0bdf-4699-ab8f-50f52ed822bd")
        )
        (fp_line
            (start -3 4.48)
            (end -3 5.4)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "2b086326-dc9e-45c4-b2b6-450bc1b63f13")
        )
        (fp_line
            (start 3 -5.6)
            (end 3 -2.48)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "df0a8a65-89bc-4e66-8e04-d032daa985b9")
        )
        (fp_line
            (start 3 -0.52)
            (end 3 3.4)
            (stroke
                (width 0.25)
                (type solid)
            )
            (layer "F.SilkS")
            (uuid "ac3a71db-10b0-4679-8ea4-a9f711c3287d")
        )
        (fp_circle
            (center -4.5 -8.6)
            (end -4.47 -8.6)
            (stroke
                (width 0.06)
                (type solid)
            )
            (fill no)
            (layer "F.Fab")
            (uuid "16be9031-eaa0-4305-9f69-5d8f7081eda9")
        )
        (fp_circle
            (center -5.26 -3.44)
            (end -5.06 -3.44)
            (stroke
                (width 0.4)
                (type solid)
            )
            (fill no)
            (layer "Cmts.User")
            (uuid "04a96ffb-c8eb-4963-be85-9a83d9bc7c8a")
        )
        (fp_circle
            (center 0 -3.6)
            (end 0.18 -3.6)
            (stroke
                (width 0.35)
                (type solid)
            )
            (fill no)
            (layer "Cmts.User")
            (uuid "4a118e83-edac-420f-90cb-a19b4c447cc7")
        )
        (fp_circle
            (center 0 2.4)
            (end 0.18 2.4)
            (stroke
                (width 0.35)
                (type solid)
            )
            (fill no)
            (layer "Cmts.User")
            (uuid "d0f8204f-b0bd-44c3-b228-c45397af3a59")
        )
        (fp_text user "%R"
            (at 0 0 0)
            (layer "F.Fab")
            (uuid "a8721c8d-23b1-466e-a33c-8b138911af4b")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (fp_text user "${REFERENCE}"
            (at 0 -7.5 0)
            (layer "F.SilkS")
            (uuid "be499d2b-ceff-42c4-ae9f-e0cf276282c3")
            (effects
                (font
                    (size 1 1)
                    (thickness 0.15)
                )
            )
            (unlocked no)
        )
        (pad "1" smd rect
            (at -4 -3.5 -90)
            (size 3 1.5)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 19 "TIP")
            (uuid "595f4fea-0483-42a8-9d8a-5a74b992a19c")
        )
        (pad "2" smd rect
            (at 4 -1.5 -90)
            (size 3 1.5)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 15 "RING")
            (uuid "cf5ebc27-970f-4acc-955c-271ca6c050c8")
        )
        (pad "3" smd rect
            (at -4 3.5 -90)
            (size 3 1.5)
            (layers "F.Cu" "F.Paste" "F.Mask")
            (net 11 "gnd")
            (uuid "ef445f3d-4228-4236-bee8-063ed64585f9")
        )
        (pad "" thru_hole circle
            (at 0 -3.6 -90)
            (size 1.3 1.3)
            (drill 1.3)
            (layers "*.Cu" "*.Mask")
            (net 21 "net")
            (uuid "00377648-1d1b-4314-b453-ce3b4d2b861c")
        )
        (pad "" thru_hole circle
            (at 0 2.4 -90)
            (size 1.3 1.3)
            (drill 1.3)
            (layers "*.Cu" "*.Mask")
            (net 21 "net")
            (uuid "f547122d-6cc1-4282-bf7b-360df81d3753")
        )
        (model "${KIPRJMOD}/../../parts/SOFNG_PJ_320B/AUDIO-PJ320B_L14.0-W6.4-H4.0.step"
            (offset
                (xyz 0 0 0.5)
            )
            (scale
                (xyz 1 1 1)
            )
            (rotate
                (xyz 0 0 0)
            )
        )
    )
    (zone
        (net 11)
        (net_name "gnd")
        (layers "F.Cu")
        (uuid "daecd2d1-61e3-42b8-9acd-6e39cb61ca6f")
        (hatch edge 0.5)
        (connect_pads
            (clearance 0.5)
        )
        (min_thickness 0.25)
        (filled_areas_thickness no)
        (fill yes
            (thermal_gap 0.5)
            (thermal_bridge_width 0.5)
        )
        (polygon
            (pts
                (xy 127 75)
                (xy 173.5 75)
                (xy 173.5 124)
                (xy 127 124)
            )
        )
    )
    (embedded_fonts no)
    (segment
        (start 159.46 97.8)
        (end 159.46 104)
        (width 0.2)
        (net 10)
        (uuid "7a6dcb04-4077-4d1f-9da0-281a017f2554")
        (layer "F.Cu")
    )
    (segment
        (start 166.26 91)
        (end 159.46 97.8)
        (width 0.2)
        (net 10)
        (uuid "a632f62f-7b5c-4be7-95db-99278b4d2806")
        (layer "F.Cu")
    )
    (segment
        (start 164.01 89)
        (end 166.26 89)
        (width 0.2)
        (net 12)
        (uuid "0f980afa-a231-4420-86ce-4749d6e22150")
        (layer "F.Cu")
    )
    (segment
        (start 156.92 96.09)
        (end 164.01 89)
        (width 0.2)
        (net 12)
        (uuid "130aa9f6-7557-4cdf-ab61-e5970230b03e")
        (layer "F.Cu")
    )
    (segment
        (start 156.92 101)
        (end 156.92 96.09)
        (width 0.2)
        (net 12)
        (uuid "c72165be-70d3-4efe-846d-829d7b3e2831")
        (layer "F.Cu")
    )
    (segment
        (start 136.49 98.6)
        (end 136.49 91.52)
        (width 0.2)
        (net 13)
        (uuid "25fe65cf-f047-4841-a7f6-9efadf76ed5f")
        (layer "F.Cu")
    )
    (segment
        (start 136.49 91.52)
        (end 136.32 91.35)
        (width 0.2)
        (net 13)
        (uuid "c38f8f4e-6bd2-49c8-a71a-2d8c42a59ab2")
        (layer "F.Cu")
    )
    (segment
        (start 160.6 120.3)
        (end 160.6 110.22)
        (width 0.2)
        (net 15)
        (uuid "0ff3f78a-f0c1-4404-b77a-07a527aed08a")
        (layer "F.Cu")
    )
    (segment
        (start 160.6 110.22)
        (end 154.38 104)
        (width 0.2)
        (net 15)
        (uuid "830bb8c2-30bc-45c7-ba21-977a55aa6447")
        (layer "F.Cu")
    )
    (segment
        (start 154.38 104)
        (end 154.802 104)
        (width 0.2)
        (net 15)
        (uuid "8fa21d88-ae6f-4900-8048-bce6f7ea3d0f")
        (layer "F.Cu")
    )
    (segment
        (start 136.51 103.4)
        (end 143.62 103.4)
        (width 0.2)
        (net 16)
        (uuid "5602c445-a5e2-4609-bfde-164083249840")
        (layer "F.Cu")
    )
    (segment
        (start 144.6 110.9)
        (end 144.6 104.38)
        (width 0.2)
        (net 16)
        (uuid "a04be25a-69f3-4ded-9eda-ed92bf73ce74")
        (layer "F.Cu")
    )
    (segment
        (start 144.6 104.38)
        (end 144.22 104)
        (width 0.2)
        (net 16)
        (uuid "c2b6b318-e411-452d-a756-d425138e431f")
        (layer "F.Cu")
    )
    (segment
        (start 143.62 103.4)
        (end 144.22 104)
        (width 0.2)
        (net 16)
        (uuid "c826683e-20ae-44a9-a306-9af2e626b409")
        (layer "F.Cu")
    )
    (segment
        (start 149.3 87.8)
        (end 146.85 85.35)
        (width 0.2)
        (net 17)
        (uuid "c0b91930-36c3-45ea-b761-bdd9e08fd371")
        (layer "F.Cu")
    )
    (segment
        (start 149.3 104)
        (end 149.3 87.8)
        (width 0.2)
        (net 17)
        (uuid "c406c41d-85d9-43c6-ab08-e633d54b94f3")
        (layer "F.Cu")
    )
    (segment
        (start 146.85 85.35)
        (end 136.32 85.35)
        (width 0.2)
        (net 17)
        (uuid "cbfd11e4-d32f-4a91-8b7e-08c261f3cefc")
        (layer "F.Cu")
    )
    (segment
        (start 152 101.16)
        (end 151.84 101)
        (width 0.2)
        (net 19)
        (uuid "0f0c2d75-ef3d-411c-9aec-97dddaeddadc")
        (layer "F.Cu")
    )
    (segment
        (start 151.84 104.34)
        (end 151.84 101)
        (width 0.2)
        (net 19)
        (uuid "5c149e74-eef2-430a-b49b-0ec76ed109b7")
        (layer "F.Cu")
    )
    (segment
        (start 152 113.3)
        (end 152 101.16)
        (width 0.2)
        (net 19)
        (uuid "dbb3947d-c2ac-4509-a44d-c4b425448134")
        (layer "F.Cu")
    )
    (segment
        (start 146.86 88)
        (end 146.86 100.9)
        (width 0.2)
        (net 22)
        (uuid "51600c06-7472-4bd7-98aa-5ad443f25d29")
        (layer "F.Cu")
    )
    (segment
        (start 146.86 100.9)
        (end 146.76 101)
        (width 0.2)
        (net 22)
        (uuid "7262a933-6a64-4529-b0a5-2ae2ccb897e6")
        (layer "F.Cu")
    )
    (segment
        (start 136.97 88)
        (end 136.32 87.35)
        (width 0.2)
        (net 23)
        (uuid "0a0a305d-e020-4696-b239-583e8f8b7aa6")
        (layer "F.Cu")
    )
    (segment
        (start 146 88)
        (end 136.97 88)
        (width 0.2)
        (net 23)
        (uuid "1a0a0928-7e8c-41be-8582-a7c4cde1a7bd")
        (layer "F.Cu")
    )
    (gr_line
        (start 126 124)
        (end 126 75)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "20cb8227-df67-4771-9d99-3d752e2b1dff")
    )
    (gr_line
        (start 173.5 125)
        (end 127 125)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "34d05532-dac1-4a7f-bfb5-3c2dce4f3322")
    )
    (gr_line
        (start 174.5 75)
        (end 174.5 124)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "762bfb10-8fc1-4111-a779-3fbce310fb4b")
    )
    (gr_line
        (start 127 74)
        (end 173.5 74)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "95502092-9d9b-41b4-8591-a8bf71a33a64")
    )
    (gr_arc
        (start 127 125)
        (mid 126.292893 124.707107)
        (end 126 124)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "3ca62288-3469-4075-8587-2421696ab497")
    )
    (gr_arc
        (start 126 75)
        (mid 126.292893 74.292893)
        (end 127 74)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "3ce3de51-baa5-4219-8d96-e12a17c4594b")
    )
    (gr_arc
        (start 174.5 124)
        (mid 174.207107 124.707107)
        (end 173.5 125)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "41b77086-ce03-4814-a34c-609cbe3e7217")
    )
    (gr_arc
        (start 173.5 74)
        (mid 174.207107 74.292893)
        (end 174.5 75)
        (stroke
            (width 0.05)
            (type default)
        )
        (layer "Edge.Cuts")
        (uuid "aa01faec-55d9-4af7-a88a-5e87bb9df99d")
    )
    (gr_rect
        (start 127 75)
        (end 173.5 124)
        (stroke
            (width 0.05)
            (type default)
        )
        (fill no)
        (layer "Edge.Cuts")
        (uuid "2c033a7d-793b-497b-afbd-893271013164")
    )
    (gr_text "DFPlayer carrier board"
        (at 131 121.5 90)
        (layer "F.Cu")
        (uuid "131bb0c9-dff7-469a-8372-f659068f6579")
        (effects
            (font
                (size 1.5 1.5)
                (thickness 0.3)
                (bold yes)
            )
            (hide no)
            (justify left bottom)
        )
    )
)