(footprint "ROQANG_RVT1A471M0607:CAP-SMD_BD6.3-L6.6-W6.6-FD"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -4 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "fd091def-bea5-40f8-ac65-a6d182e98eee")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "CAP-SMD_BD6.3-L6.6-W6.6-FD"
        (at 0 4 0)
        (layer "F.Fab")
        (hide no)
        (uuid "275a3428-2722-47cb-a486-a03ac350f381")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "checksum" "ac6d86359670df5b4e5c2ac739e549161f887eb409f3546f17493db0a046ae3c"
        (at 0 0 0)
        (layer "User.9")
        (hide no)
        (uuid "99234980-dd78-417f-9dfb-e8dbb447bbf5")
        (effects
            (font
                (size 0.125 0.125)
                (thickness 0.01875)
            )
            (hide yes)
        )
    )
    (attr smd)
    (fp_line
        (start 3.36 0.74)
        (end 3.38 3.38)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "c0c04a2d-4d76-4187-8b20-8cc7e1c2f79a")
    )
    (fp_line
        (start 3.38 3.38)
        (end -1.98 3.38)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "e9173faf-b5d8-4728-82e0-17c9f3338376")
    )
    (fp_line
        (start -1.98 3.38)
        (end -3.38 1.98)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "15bbf761-eb87-4ccc-ac91-10133813285d")
    )
    (fp_line
        (start -3.38 1.98)
        (end -3.36 0.69)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "aae84088-947a-4619-b2c9-1af38abdf506")
    )
    (fp_line
        (start 3.37 -0.71)
        (end 3.38 -3.38)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "aaaabbf4-1c3c-4a88-9d59-e6ecf46a613c")
    )
    (fp_line
        (start 3.38 -3.38)
        (end -1.98 -3.38)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "c4eeed76-f3a6-4a60-a7e0-6f2441d0411b")
    )
    (fp_line
        (start -1.98 -3.38)
        (end -3.38 -1.98)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "a885ee70-010e-481d-bf52-662ab54e9f26")
    )
    (fp_line
        (start -3.38 -1.98)
        (end -3.38 -0.69)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "79885ee0-7260-4b85-9419-0c98bf4b9a57")
    )
    (fp_circle
        (center -3.63 3.3)
        (end -3.6 3.3)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "34ad77bc-7933-4e89-9a5f-e6bdf28c865f")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "ce009cbe-0092-4151-888c-74fad6c93e55")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -4 0)
        (layer "F.SilkS")
        (uuid "fd091def-bea5-40f8-ac65-a6d182e98eee")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "1" smd rect
        (at -2.67 0 0)
        (size 3.5 1.2)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "6890359e-f9e7-4e0f-8f1e-d281e2f7e18a")
    )
    (pad "2" smd rect
        (at 2.67 0 0)
        (size 3.5 1.2)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "476dae52-0d0b-4d0f-9ceb-6850597e6450")
    )
    (model "${KIPRJMOD}/../../parts/ROQANG_RVT1A471M0607/CAP-SMD_BD6.3-L6.6-W6.6-FD.step"
        (offset
            (xyz 0 0 0)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 180)
        )
    )
)