(footprint "SOFNG_PJ_320B:AUDIO-SMD_PJ-320B"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -7.5 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "be499d2b-ceff-42c4-ae9f-e0cf276282c3")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "AUDIO-SMD_PJ-320B"
        (at 0 7.5 0)
        (layer "F.Fab")
        (hide no)
        (uuid "dc5db5a9-a1f7-42df-ab7f-aff4f953b13d")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "checksum" "985abb5c5ae306cde70e644fc7a519056db632b07114d61a7ce01ffd2efb0f20"
        (at 0 0 0)
        (layer "User.9")
        (hide no)
        (uuid "62af287f-ee27-43c3-b5c5-76d8ba513648")
        (effects
            (font
                (size 0.125 0.125)
                (thickness 0.01875)
            )
            (hide yes)
        )
    )
    (attr smd)
    (fp_line
        (start -3 -5.6)
        (end 3 -5.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "84248522-c4c8-44ef-bce2-3232672fca83")
    )
    (fp_line
        (start 3 5.4)
        (end -3 5.4)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "b6f9dfac-df11-449e-9984-ba472b91b69d")
    )
    (fp_line
        (start -2.5 -5.6)
        (end -2.5 -8.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "2ab5d2b9-b593-41b7-ba1e-e8bddb1cdc55")
    )
    (fp_line
        (start -2.5 -8.6)
        (end 2.5 -8.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "3c991bb5-e6f6-4fbe-81d0-a8a1304b224a")
    )
    (fp_line
        (start 2.5 -5.6)
        (end 2.5 -8.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "58fae45d-82d6-4f47-8283-8a338d54815b")
    )
    (fp_line
        (start 3 3.4)
        (end 2.3 3.4)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "c44a98ba-c637-46b3-8349-b7ab4c73ac34")
    )
    (fp_line
        (start 2.3 3.4)
        (end 2.3 4.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "1a67b0d7-8d92-42b7-8ad5-e9083258ece1")
    )
    (fp_line
        (start 2.3 4.6)
        (end 3 4.6)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "01d86d62-72e1-44c9-b0ba-64c53c7c5bde")
    )
    (fp_line
        (start 3 4.6)
        (end 3 5.4)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "13bd1d5a-7877-4165-8a30-6e8f656248d1")
    )
    (fp_line
        (start -3 -5.6)
        (end -3 -4.48)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "d5753a7b-184c-4f0f-ba0f-de057b658fa1")
    )
    (fp_line
        (start -3 -2.52)
        (end -3 2.52)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "fcddfa29-0bdf-4699-ab8f-50f52ed822bd")
    )
    (fp_line
        (start -3 4.48)
        (end -3 5.4)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "2b086326-dc9e-45c4-b2b6-450bc1b63f13")
    )
    (fp_line
        (start 3 -5.6)
        (end 3 -2.48)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "df0a8a65-89bc-4e66-8e04-d032daa985b9")
    )
    (fp_line
        (start 3 -0.52)
        (end 3 3.4)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "ac3a71db-10b0-4679-8ea4-a9f711c3287d")
    )
    (fp_circle
        (center -4.5 -8.6)
        (end -4.47 -8.6)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "16be9031-eaa0-4305-9f69-5d8f7081eda9")
    )
    (fp_circle
        (center -5.26 -3.44)
        (end -5.06 -3.44)
        (stroke
            (width 0.4)
            (type solid)
        )
        (fill no)
        (layer "Cmts.User")
        (uuid "04a96ffb-c8eb-4963-be85-9a83d9bc7c8a")
    )
    (fp_circle
        (center 0 -3.6)
        (end 0.18 -3.6)
        (stroke
            (width 0.35)
            (type solid)
        )
        (fill no)
        (layer "Cmts.User")
        (uuid "4a118e83-edac-420f-90cb-a19b4c447cc7")
    )
    (fp_circle
        (center 0 2.4)
        (end 0.18 2.4)
        (stroke
            (width 0.35)
            (type solid)
        )
        (fill no)
        (layer "Cmts.User")
        (uuid "d0f8204f-b0bd-44c3-b228-c45397af3a59")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "a8721c8d-23b1-466e-a33c-8b138911af4b")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -7.5 0)
        (layer "F.SilkS")
        (uuid "be499d2b-ceff-42c4-ae9f-e0cf276282c3")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "1" smd rect
        (at -4 -3.5 0)
        (size 3 1.5)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "595f4fea-0483-42a8-9d8a-5a74b992a19c")
    )
    (pad "2" smd rect
        (at 4 -1.5 0)
        (size 3 1.5)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "cf5ebc27-970f-4acc-955c-271ca6c050c8")
    )
    (pad "3" smd rect
        (at -4 3.5 0)
        (size 3 1.5)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "ef445f3d-4228-4236-bee8-063ed64585f9")
    )
    (pad "" thru_hole circle
        (at 0 -3.6 0)
        (size 1.3 1.3)
        (drill 1.3)
        (layers "*.Cu" "*.Mask")
        (uuid "00377648-1d1b-4314-b453-ce3b4d2b861c")
    )
    (pad "" thru_hole circle
        (at 0 2.4 0)
        (size 1.3 1.3)
        (drill 1.3)
        (layers "*.Cu" "*.Mask")
        (uuid "f547122d-6cc1-4282-bf7b-360df81d3753")
    )
    (model "${KIPRJMOD}/../../parts/SOFNG_PJ_320B/AUDIO-PJ320B_L14.0-W6.4-H4.0.step"
        (offset
            (xyz 0 0 0.5)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 0)
        )
    )
)