(footprint "MDD_Microdiode_Electronics_SM4007PL:SOD-123F_L2.8-W1.8-LS3.7-RD"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -4 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "d4d2eaf6-9211-4c52-9cb2-933df7ba6604")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "SOD-123F_L2.8-W1.8-LS3.7-RD"
        (at 0 4 0)
        (layer "F.Fab")
        (hide no)
        (uuid "2b2b20a4-2ad9-4bf2-84e3-b2943f55dff5")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "checksum" "070fa4f55c35c285219094ffce18e03cd185d39ca50a8e4ec03352c2320a53a5"
        (at 0 0 0)
        (layer "User.9")
        (hide no)
        (uuid "1a96ceb5-80c9-48ef-a131-2ad8282e06bc")
        (effects
            (font
                (size 0.125 0.125)
                (thickness 0.01875)
            )
            (hide yes)
        )
    )
    (attr smd)
    (fp_line
        (start -1.52 -0.94)
        (end 1.48 -0.94)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "d5ae25db-a483-449b-ad7a-f54444e30636")
    )
    (fp_line
        (start -1.51 0.94)
        (end 1.49 0.94)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "0acdd9a9-7a82-4b4d-8e3c-78d831c4aac1")
    )
    (fp_line
        (start -0.76 0)
        (end 0.76 0)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "cdd66404-99d6-47b0-b423-beae9108bf4e")
    )
    (fp_line
        (start -0.51 -0.5)
        (end -0.51 0.51)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "dd88475d-7ade-46be-8eff-569e7ec272a0")
    )
    (fp_line
        (start 0.51 0.41)
        (end -0.51 0)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "49e9a8ca-7a56-4ac6-b630-ab9b75d3dcb9")
    )
    (fp_line
        (start 0.51 -0.4)
        (end 0.51 0.41)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "33076ae7-6a0b-4255-9ad3-8e8beb0a40ae")
    )
    (fp_line
        (start -0.51 0)
        (end 0.51 -0.4)
        (stroke
            (width 0.25)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "68309971-6a51-4565-b170-935fcf0430bc")
    )
    (fp_circle
        (center -1.85 0.85)
        (end -1.82 0.85)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "f37c75c0-2604-4038-82d8-62d9f6a564ba")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "f5330701-f571-4d52-b6dc-8f00d8569e63")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -4 0)
        (layer "F.SilkS")
        (uuid "d4d2eaf6-9211-4c52-9cb2-933df7ba6604")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "2" smd rect
        (at 1.55 0 0)
        (size 1 1.2)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "6faf8a53-b13e-4a24-ac84-3ce8c30ae7b1")
    )
    (pad "1" smd rect
        (at -1.55 0 0)
        (size 1 1.2)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "64591f99-74ac-4520-997f-d74795eaa7f7")
    )
    (model "${KIPRJMOD}/../../parts/MDD_Microdiode_Electronics_SM4007PL/SOD-123FL_L2.8-W1.8-LS3.7-RD-1.STEP"
        (offset
            (xyz 0 0 0)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 0)
        )
    )
)