(footprint "easyeda2kicad:R0805"
    (layer "F.Cu")
    (descr "")
    (version 20241229)
    (generator "faebryk")
    (generator_version "v5")
    (tedit "5DC5F6A4")
    (property "Reference" "REF**"
        (at 0 -4 0)
        (layer "F.SilkS")
        (hide no)
        (uuid "abfc4eff-2d13-4fb2-bc5b-5c3c87bacb42")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (property "Value" "R0805"
        (at 0 4 0)
        (layer "F.Fab")
        (hide no)
        (uuid "95564364-ab35-4a94-9159-3802051a7d1a")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
    )
    (attr smd)
    (fp_line
        (start 0.48 0.92)
        (end 1.76 0.92)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "31635535-3039-4ce7-9775-9fd0201f214c")
    )
    (fp_line
        (start 1.76 0.92)
        (end 1.76 -0.92)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "0dee744d-6193-42ad-b001-5d2e18dcf7f0")
    )
    (fp_line
        (start 1.76 -0.92)
        (end 0.48 -0.92)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "380f5073-f1f3-44ae-875b-885b666d69a2")
    )
    (fp_line
        (start -0.48 0.92)
        (end -1.76 0.92)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "5d72f94f-48fd-4791-982c-09efbc097df8")
    )
    (fp_line
        (start -1.76 0.92)
        (end -1.76 -0.92)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "94885d16-be97-4fcd-aebc-44253a5ef8c0")
    )
    (fp_line
        (start -1.76 -0.92)
        (end -0.48 -0.92)
        (stroke
            (width 0.15)
            (type solid)
        )
        (layer "F.SilkS")
        (uuid "61e3e26b-54c7-4667-8a46-a48e5202803f")
    )
    (fp_circle
        (center -1 0.64)
        (end -0.97 0.64)
        (stroke
            (width 0.06)
            (type solid)
        )
        (fill no)
        (layer "F.Fab")
        (uuid "6c7d0f49-2ffa-46f5-8b13-7ca40c2d4edc")
    )
    (fp_text user "%R"
        (at 0 0 0)
        (layer "F.Fab")
        (uuid "a09f9864-259d-493b-95a7-3572dbe0263c")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (fp_text user "${REFERENCE}"
        (at 0 -4 0)
        (layer "F.SilkS")
        (uuid "abfc4eff-2d13-4fb2-bc5b-5c3c87bacb42")
        (effects
            (font
                (size 1 1)
                (thickness 0.15)
            )
        )
        (unlocked no)
    )
    (pad "2" smd rect
        (at 1 0 0)
        (size 1.13 1.38)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "0fd10d99-80da-4765-93fc-af257bbf4ad6")
    )
    (pad "1" smd rect
        (at -1 0 0)
        (size 1.13 1.38)
        (layers "F.Cu" "F.Paste" "F.Mask")
        (uuid "e7a49127-8ca6-4706-907e-6a0bb3ab1999")
    )
    (model "${KIPRJMOD}/../../build/cache/parts/easyeda/C17513/R0805_L2.0-W1.3-H0.6.step"
        (offset
            (xyz 0 0 0)
        )
        (scale
            (xyz 1 1 1)
        )
        (rotate
            (xyz 0 0 0)
        )
    )
)