(footprint "XL7015_step_down_module"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "bc12ad76-3a01-4bf9-80dd-60bb701c3524")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "XL7015_step_down_module"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "8b81088b-0b97-4bbb-8886-1ea9abf9e67f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "695c7d0f-f30e-43c7-8285-c863575aee72")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "99516c6b-c28c-4207-be18-71cb162c0836")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -22 -8)
		(end 22 8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "aa26581d-f016-42e7-bccb-e0a7db1a920e")
	)
	(fp_text user "GND"
		(at -17.5 6.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3aa866da-05da-4adf-9eb7-fcc415a2d8ff")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "VOUT"
		(at 14 -5.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "aa04dd77-fc4c-4a5f-8ba6-5001df94ef6a")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GND"
		(at 14.5 6.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "d0977f17-4df6-4619-a728-b25fd9195273")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "VIN"
		(at -17.5 -5.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e325c9b0-3b64-47e9-879e-75edb532fbcc")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "09714687-21bd-4280-8f07-b2e1324633e9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -19.5 -6.125)
		(size 2.5 2.5)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a6c37468-d638-4770-8e7f-e65f9ef72f7c")
	)
	(pad "2" thru_hole circle
		(at -19.5 6.125)
		(size 2.5 2.5)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d89f8519-63b0-458b-82ec-c473758caea8")
	)
	(pad "3" thru_hole circle
		(at 19.5 -6.125)
		(size 2.5 2.5)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9aa08891-3e3c-495f-8233-94a1b1b392c7")
	)
	(pad "4" thru_hole circle
		(at 19.5 6.125)
		(size 2.5 2.5)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d56a9c30-f1a4-43ab-a09f-b1af0e28eaaf")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(uuid "1a960a97-a485-47b5-a7d1-dccbc92e1ae3")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -22 -8) (xy 22 -8) (xy 22 8) (xy -22 8)
			)
		)
	)
	(embedded_fonts no)
)
